*** Creating Trace Output File '.\Output\UART.tra' Ok.
### Preparing for ADS-LD.
### Creating ADS-LD Command Line
### List of Objects: adding '".\output\startup.o"'
### List of Objects: adding '".\output\pcd5544.o"'
### List of Objects: adding '".\output\uart_echo.o"'
### List of Objects: adding '"C:\Keil\ARM\RV31\LIB\Luminary\DriverLib.lib"'
### List of Objects: adding '".\output\uart.o"'
### ADS-LD Command completed:
".\output\startup.o" ".\output\pcd5544.o" ".\output\uart_echo.o" "C:\Keil\ARM\RV31\LIB\Luminary\DriverLib.lib" ".\output\uart.o" --device DLM --strict --scatter ".\Output\UART.sct" 

--autoat --summary_stderr --info summarysizes --map --xref --callgraph --symbols 

--info sizes --info totals --info unused --info veneers 

 --list ".\Output\UART.map" -o ".\Output\UART.axf"### Preparing Environment (PrepEnvAds)
### ADS-LD Output File: '.\Output\UART.axf'
### ADS-LD Command File: '.\Output\UART.lnp'
### Checking for dirty Components...
### Creating CmdFile '.\Output\UART.lnp', Handle=0x00000294
### Writing '.lnp' file
### ADS-LD Command file '.\Output\UART.lnp' is ready.
### ADS-LD: About to start ADS-LD Thread.
### ADS-LD: executed with 0 errors
### Updating obj list
### LDADS_file() completed.
