#

##

##

    µVision3 Build Log
    Project:
    C:\zero\LPC2148V2\Example\USB ISP\USBMem\Memory.uv2
    Project File Date:  03/24/2009

    Output:
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.
    Build target 'MCB2140 Board'
    assembling Startup.s...
    compiling DiskImg.c...
    compiling usbhw.c...
    compiling usbcore.c...
    usbcore.c(323): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: msk may be used before being set
    usbcore.c(405): warning: C3017W: old may be used before being set
    usbcore.c(405): warning: C3017W: alt may be used before being set
    usbcore.c(405): warning: C3017W: ifn may be used before being set
    compiling usbdesc.c...
    compiling usbuser.c...
    compiling mscuser.c...
    compiling memory.c...
    compiling sbl_iap.c...
    linking...
    Program Size: Code=6616 RO-data=620 RW-data=68 ZI-data=5244
    FromELF: creating hex file...
    ".\Obj\Memory.axf" - 0 Error(s), 5 Warning(s).
    Load "C:\\zero\\LPC2148V2\\Example\\USB ISP\\USBMem\\Obj\\Memory.AXF"
    Erase Done.
    Programming Done.
    Verify OK.