R E V I S I O N   H I S T O R Y

Product:	EZMac(TM) Lite

Version 1.8 (Sep 29,2006)
=========================
- EZMacBuf_Read is only possible when EZMac is in either Idle or in PacketValid states

Version 1.7 (Dec 09,2005)
=========================
- Transfer under Hitech C, CCS is not supported
- Supports standard baud rates from 9600bps to 115.2bps
- Supports the following ISM bands: 315MHz, 433MHz, 868MHz, 915MHz
- ARSSI measurement improvement


Version 1.6 (Aug 11,2005)
=========================
Initial Public Release
Created from EZMac(TM) 1.6 by removing the following features:
	- Multicast addressing
	- Network address mode
	- Reduced address mode
	- Dynamic packet length
	- Error detection
	- CID is mandatory.  


