; generated by ARM C/C++ Compiler, 5.03 [Build 24]
; commandline ArmCC [--list --debug -c --asm --interleave -o..\OBJ\core_cm3.o --asm_dir=..\LIST\ --list_dir=..\LIST\ --depend=..\OBJ\core_cm3.d --cpu=Cortex-M3 --apcs=interwork -O0 -I..\..\Libraries\STM32F10x_StdPeriph_Driver\inc -I..\..\Libraries\CMSIS\CM3\CoreSupport -I..\..\Libraries\CMSIS\CM3\DeviceSupport\ST\STM32F10x -I..\..\USER\INC -IC:\Keil\ARM\RV31\INC -IC:\Keil\ARM\CMSIS\Include -IC:\Keil\ARM\Inc\ST\STM32F10x -D__MICROLIB -DUSE_STDPERIPH_DRIVER -DSTM32F10X_HD --omf_browse=..\OBJ\core_cm3.crf ..\..\Libraries\CMSIS\CM3\CoreSupport\core_cm3.c]
                          THUMB

;*** Start embedded assembler ***

#line 1 "..\\..\\Libraries\\CMSIS\\CM3\\CoreSupport\\core_cm3.c"
	AREA ||.emb_text||, CODE, READONLY
	THUMB
	EXPORT |__get_PSP|
#line 58
|__get_PSP| PROC
#line 59

 mrs r0, psp
 bx lr
	ENDP
	AREA ||.emb_text||, CODE, READONLY
	THUMB
	EXPORT |__set_PSP|
#line 72
|__set_PSP| PROC
#line 73

 msr psp, r0
 bx lr
	ENDP
	AREA ||.emb_text||, CODE, READONLY
	THUMB
	EXPORT |__get_MSP|
#line 86
|__get_MSP| PROC
#line 87

 mrs r0, msp
 bx lr
	ENDP
	AREA ||.emb_text||, CODE, READONLY
	THUMB
	EXPORT |__set_MSP|
#line 100
|__set_MSP| PROC
#line 101

 msr msp, r0
 bx lr
	ENDP
	AREA ||.emb_text||, CODE, READONLY
	THUMB
	EXPORT |__REV16|
#line 114
|__REV16| PROC
#line 115

 rev16 r0, r0
 bx lr
	ENDP
	AREA ||.emb_text||, CODE, READONLY
	THUMB
	EXPORT |__REVSH|
#line 128
|__REVSH| PROC
#line 129

 revsh r0, r0
 bx lr
	ENDP

;*** End   embedded assembler ***
