# Static Call Graph for image .\keil_output\iflash_nxp_xpresso_812\freertos_blinky_iflash_nxp_xpresso_812.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 69]: Last Updated: Fri May 31 15:31:52 2013

### Maximum Stack Usage = 160 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ vTaskStartScheduler ⇒ xTaskGenericCreate ⇒ pvPortMalloc ⇒ malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- HardFault_Handler ⇒ HardFault_Handler
- BOD_IRQHandler ⇒ BOD_IRQHandler

  ### Function Pointers

  - BOD_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - CMP_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - FLASH_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - HardFault_Handler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - I2C_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - MRT_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - NMI_Handler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT0_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT1_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT2_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT3_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT4_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT5_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT6_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - PININT7_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - Reset_Handler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - SCT_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - SPI0_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - SPI1_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - SystemInit from sysinit_nxp_xpresso_812.o(i.SystemInit) referenced from keil_freertos_startup_lpc8xx.o(.text)
  - UART0_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - UART1_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - UART2_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - WDT_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - WKT_IRQHandler from keil_freertos_startup_lpc8xx.o(.text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - __main from __main.o(!!!main) referenced from keil_freertos_startup_lpc8xx.o(.text)
  - prvIdleTask from tasks.o(i.prvIdleTask) referenced from tasks.o(i.vTaskStartScheduler)
  - vLEDTask0 from freertos_blinky.o(i.vLEDTask0) referenced from freertos_blinky.o(i.main)
  - vLEDTask1 from freertos_blinky.o(i.vLEDTask1) referenced from freertos_blinky.o(i.main)
  - vLEDTask2 from freertos_blinky.o(i.vLEDTask2) referenced from freertos_blinky.o(i.main)
  - vPortSVCHandler from port_m0.o(.emb_text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - xPortPendSVHandler from port_m0.o(.emb_text) referenced from keil_freertos_startup_lpc8xx.o(RESET)
  - xPortSysTickHandler from port_m0.o(i.xPortSysTickHandler) referenced from keil_freertos_startup_lpc8xx.o(RESET)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 52 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000001))

  __rt_lib_init_heap_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000003))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = __rt_lib_init_heap_2 ⇒ _init_alloc ⇒ __rt_SIGRTMEM ⇒ __rt_SIGRTMEM_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> _init_alloc

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ vTaskStartScheduler ⇒ xTaskGenericCreate ⇒ pvPortMalloc ⇒ malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  vPortSVCHandler (Thumb, 34 bytes, Stack size 0 bytes, port_m0.o(.emb_text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  vPortStartFirstTask (Thumb, 14 bytes, Stack size 0 bytes, port_m0.o(.emb_text))
  [Called By]

  - >> xPortStartScheduler

  xPortPendSVHandler (Thumb, 62 bytes, Stack size 0 bytes, port_m0.o(.emb_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = xPortPendSVHandler ⇒ vTaskSwitchContext ⇒ memcmp
  [Calls]
  - >> vTaskSwitchContext
  [Address Reference Count : 1]
  - keil_freertos_startup_lpc8xx.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  _maybe_terminate_alloc (Thumb, 0 bytes, Stack size 0 bytes, maybetermalloc1.o(.emb_text), UNUSED)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - keil_freertos_startup_lpc8xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text), UNUSED)
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text), UNUSED)
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text), UNUSED)
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Calls]

  - >> BOD_IRQHandler
  [Called By]
  - >> BOD_IRQHandler
  [Address Reference Count : 1]
  - keil_freertos_startup_lpc8xx.o(RESET)

  CMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  I2C_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  MRT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  NMI_Handler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  PININT7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  SCT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  WKT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Address Reference Count : 1]

  - keil_freertos_startup_lpc8xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, keil_freertos_startup_lpc8xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  malloc (Thumb, 98 bytes, Stack size 16 bytes, h1_alloc.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> __Heap_Full
  - >> __rt_heap_descriptor
  [Called By]
  - >> pvPortMalloc

  free (Thumb, 76 bytes, Stack size 16 bytes, h1_free.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = free
  [Calls]
  - >> __rt_heap_descriptor
  [Called By]
  - >> vPortFree
  - >> __Heap_ProvideMemory

  memcmp (Thumb, 90 bytes, Stack size 8 bytes, memcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = memcmp
  [Called By]
  - >> vTaskSwitchContext

  __aeabi_memset (Thumb, 18 bytes, Stack size 8 bytes, aeabi_memset.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_memset
  [Calls]
  - >> _memset
  [Called By]
  - >> xTaskGenericCreate

  strncpy (Thumb, 104 bytes, Stack size 24 bytes, strncpy.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = strncpy
  [Calls]
  - >> __rt_memclr
  [Called By]
  - >> xTaskGenericCreate

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 20 bytes, Stack size 0 bytes, aeabi_sdiv.o(.text))
  [Called By]

  - >> xPortStartScheduler
  - >> Chip_Clock_GetWDTOSCRate
  - >> Chip_Clock_GetSystemClockRate

  __aeabi_idiv (Thumb, 0 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __aeabi_idivmod (Thumb, 326 bytes, Stack size 8 bytes, aeabi_sdiv.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_descriptor (Thumb, 8 bytes, Stack size 0 bytes, rt_heap_descriptor_intlibspace.o(.text))
  [Called By]

  - >> free
  - >> malloc
  - >> _init_alloc

  __use_no_heap (Thumb, 2 bytes, Stack size 0 bytes, hguard.o(.text), UNUSED)

  __heap$guard (Thumb, 2 bytes, Stack size 0 bytes, hguard.o(.text), UNUSED)

  _terminate_user_alloc (Thumb, 2 bytes, Stack size 0 bytes, init_alloc.o(.text), UNUSED)

  _init_user_alloc (Thumb, 2 bytes, Stack size 0 bytes, init_alloc.o(.text), UNUSED)

  __Heap_Full (Thumb, 32 bytes, Stack size 16 bytes, init_alloc.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> __Heap_ProvideMemory
  [Called By]
  - >> malloc

  __Heap_Broken (Thumb, 10 bytes, Stack size 8 bytes, init_alloc.o(.text), UNUSED)
  [Calls]

  - >> __rt_SIGRTMEM

  _init_alloc (Thumb, 90 bytes, Stack size 24 bytes, init_alloc.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _init_alloc ⇒ __rt_SIGRTMEM ⇒ __rt_SIGRTMEM_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> __rt_SIGRTMEM
  - >> __Heap_ProvideMemory
  - >> __Heap_Initialize
  - >> __rt_heap_descriptor
  [Called By]
  - >> __rt_lib_init_heap_2

  __Heap_Initialize (Thumb, 10 bytes, Stack size 0 bytes, h1_init.o(.text))
  [Called By]

  - >> _init_alloc

  __Heap_DescSize (Thumb, 4 bytes, Stack size 0 bytes, h1_init.o(.text), UNUSED)

  _memset_w (Thumb, 26 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Called By]

  - >> __rt_memclr_w
  - >> _memset

  _memset (Thumb, 30 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Calls]

  - >> _memset_w
  [Called By]
  - >> __aeabi_memclr
  - >> __aeabi_memset

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset

  __rt_memclr (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Called By]

  - >> strncpy

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 4 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset_w

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __Heap_ProvideMemory (Thumb, 52 bytes, Stack size 8 bytes, h1_extend.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> free
  [Called By]
  - >> _init_alloc
  - >> __Heap_Full

  __rt_SIGRTMEM (Thumb, 12 bytes, Stack size 8 bytes, defsig_rtmem_outer.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __rt_SIGRTMEM ⇒ __rt_SIGRTMEM_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> __rt_SIGRTMEM_inner
  - >> __sig_exit
  [Called By]
  - >> _init_alloc
  - >> __Heap_Broken

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 8 bytes, indicate_semi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 62 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  - >> _call_atexit_fns (Weak Reference)
  [Called By]
  - >> __rt_entry_main

  __sig_exit (Thumb, 12 bytes, Stack size 8 bytes, defsig_exit.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __sig_exit
  [Calls]
  - >> _sys_exit
  [Called By]
  - >> __rt_SIGRTMEM

  __rt_SIGRTMEM_inner (Thumb, 22 bytes, Stack size 8 bytes, defsig_rtmem_inner.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = __rt_SIGRTMEM_inner ⇒ __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> __default_signal_display
  [Called By]
  - >> __rt_SIGRTMEM

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit
  - >> __sig_exit

  __default_signal_display (Thumb, 52 bytes, Stack size 16 bytes, defsig_general.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = __default_signal_display ⇒ _ttywrch
  [Calls]
  - >> _ttywrch
  [Called By]
  - >> __rt_SIGRTMEM_inner

  _ttywrch (Thumb, 12 bytes, Stack size 8 bytes, sys_wrch.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _ttywrch
  [Called By]
  - >> __default_signal_display

  Board_Init (Thumb, 12 bytes, Stack size 8 bytes, board_nxp_xpresso_812.o(i.Board_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = Board_Init ⇒ SystemCoreClockUpdate ⇒ Chip_Clock_GetSystemClockRate ⇒ Chip_Clock_GetMainClockRate ⇒ Chip_Clock_GetWDTOSCRate
  [Calls]
  - >> SystemCoreClockUpdate
  - >> Board_LED_Init
  [Called By]
  - >> main

  Board_LED_Set (Thumb, 16 bytes, Stack size 0 bytes, board_nxp_xpresso_812.o(i.Board_LED_Set))
  [Called By]

  - >> vLEDTask2
  - >> vLEDTask1
  - >> vLEDTask0

  Chip_Clock_GetMainClockRate (Thumb, 48 bytes, Stack size 8 bytes, clock_8xx.o(i.Chip_Clock_GetMainClockRate))
  [Stack]

  - Max Depth = 16
  - Call Chain = Chip_Clock_GetMainClockRate ⇒ Chip_Clock_GetWDTOSCRate
  [Calls]
  - >> Chip_Clock_GetWDTOSCRate
  - >> Chip_Clock_GetSystemPllOutClockRate
  - >> Chip_Clock_GetSystemPllInClockRate
  [Called By]
  - >> Chip_Clock_GetSystemClockRate

  Chip_Clock_GetSystemClockRate (Thumb, 16 bytes, Stack size 8 bytes, clock_8xx.o(i.Chip_Clock_GetSystemClockRate))
  [Stack]

  - Max Depth = 24
  - Call Chain = Chip_Clock_GetSystemClockRate ⇒ Chip_Clock_GetMainClockRate ⇒ Chip_Clock_GetWDTOSCRate
  [Calls]
  - >> Chip_Clock_GetMainClockRate
  - >> __aeabi_uidivmod
  [Called By]
  - >> SystemCoreClockUpdate

  Chip_Clock_GetSystemPllInClockRate (Thumb, 20 bytes, Stack size 0 bytes, clock_8xx.o(i.Chip_Clock_GetSystemPllInClockRate))
  [Called By]

  - >> Chip_Clock_GetSystemPllOutClockRate
  - >> Chip_Clock_GetMainClockRate

  Chip_Clock_GetSystemPllOutClockRate (Thumb, 20 bytes, Stack size 4 bytes, clock_8xx.o(i.Chip_Clock_GetSystemPllOutClockRate))
  [Stack]

  - Max Depth = 4
  - Call Chain = Chip_Clock_GetSystemPllOutClockRate
  [Calls]
  - >> Chip_Clock_GetSystemPllInClockRate
  [Called By]
  - >> Chip_Clock_GetMainClockRate

  Chip_Clock_GetWDTOSCRate (Thumb, 28 bytes, Stack size 8 bytes, clock_8xx.o(i.Chip_Clock_GetWDTOSCRate))
  [Stack]

  - Max Depth = 8
  - Call Chain = Chip_Clock_GetWDTOSCRate
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> Chip_Clock_GetMainClockRate

  Chip_Clock_SetCLKOUTSource (Thumb, 16 bytes, Stack size 0 bytes, clock_8xx.o(i.Chip_Clock_SetCLKOUTSource))
  [Called By]

  - >> SystemSetupClocking

  Chip_Clock_SetMainClockSource (Thumb, 14 bytes, Stack size 0 bytes, clock_8xx.o(i.Chip_Clock_SetMainClockSource))
  [Called By]

  - >> SystemSetupClocking

  Chip_Clock_SetPLLBypass (Thumb, 22 bytes, Stack size 0 bytes, clock_8xx.o(i.Chip_Clock_SetPLLBypass))
  [Called By]

  - >> SystemSetupClocking

  Chip_Clock_SetSystemPllSource (Thumb, 14 bytes, Stack size 0 bytes, clock_8xx.o(i.Chip_Clock_SetSystemPllSource))
  [Called By]

  - >> SystemSetupClocking

  Chip_SYSCTL_PowerUp (Thumb, 20 bytes, Stack size 0 bytes, syscon_8xx.o(i.Chip_SYSCTL_PowerUp))
  [Called By]

  - >> SystemSetupClocking

  SystemCoreClockUpdate (Thumb, 12 bytes, Stack size 8 bytes, board_nxp_xpresso_812.o(i.SystemCoreClockUpdate))
  [Stack]

  - Max Depth = 32
  - Call Chain = SystemCoreClockUpdate ⇒ Chip_Clock_GetSystemClockRate ⇒ Chip_Clock_GetMainClockRate ⇒ Chip_Clock_GetWDTOSCRate
  [Calls]
  - >> Chip_Clock_GetSystemClockRate
  [Called By]
  - >> Board_Init

  SystemInit (Thumb, 80 bytes, Stack size 8 bytes, sysinit_nxp_xpresso_812.o(i.SystemInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SystemSetupClocking
  [Calls]
  - >> SystemSetupClocking
  - >> Chip_Clock_EnablePeriphClock
  [Address Reference Count : 1]
  - keil_freertos_startup_lpc8xx.o(.text)

  main (Thumb, 80 bytes, Stack size 32 bytes, freertos_blinky.o(i.main))
  [Stack]

  - Max Depth = 160
  - Call Chain = main ⇒ vTaskStartScheduler ⇒ xTaskGenericCreate ⇒ pvPortMalloc ⇒ malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> xTaskGenericCreate
  - >> vTaskStartScheduler
  - >> Board_Init
  [Called By]
  - >> __rt_entry_main

  pvPortMalloc (Thumb, 32 bytes, Stack size 8 bytes, heap_3.o(i.pvPortMalloc))
  [Stack]

  - Max Depth = 64
  - Call Chain = pvPortMalloc ⇒ malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> xTaskResumeAll
  - >> vTaskSuspendAll
  - >> malloc
  - >> vApplicationMallocFailedHook
  [Called By]
  - >> xTaskGenericCreate

  pxPortInitialiseStack (Thumb, 24 bytes, Stack size 8 bytes, port_m0.o(i.pxPortInitialiseStack))
  [Stack]

  - Max Depth = 8
  - Call Chain = pxPortInitialiseStack
  [Called By]
  - >> xTaskGenericCreate

  uxListRemove (Thumb, 38 bytes, Stack size 0 bytes, list.o(i.uxListRemove))
  [Called By]

  - >> xTaskResumeAll
  - >> vTaskIncrementTick
  - >> prvCheckTasksWaitingTermination
  - >> vTaskDelay

  vApplicationIdleHook (Thumb, 4 bytes, Stack size 0 bytes, freertoscommonhooks.o(i.vApplicationIdleHook))
  [Called By]

  - >> prvIdleTask

  vApplicationMallocFailedHook (Thumb, 4 bytes, Stack size 0 bytes, freertoscommonhooks.o(i.vApplicationMallocFailedHook))
  [Called By]

  - >> pvPortMalloc

  vApplicationStackOverflowHook (Thumb, 4 bytes, Stack size 0 bytes, freertoscommonhooks.o(i.vApplicationStackOverflowHook))
  [Called By]

  - >> vTaskSwitchContext

  vListInitialise (Thumb, 22 bytes, Stack size 0 bytes, list.o(i.vListInitialise))
  [Called By]

  - >> xTaskGenericCreate

  vListInitialiseItem (Thumb, 6 bytes, Stack size 0 bytes, list.o(i.vListInitialiseItem))
  [Called By]

  - >> xTaskGenericCreate

  vListInsert (Thumb, 48 bytes, Stack size 8 bytes, list.o(i.vListInsert))
  [Stack]

  - Max Depth = 8
  - Call Chain = vListInsert
  [Called By]
  - >> prvAddCurrentTaskToDelayedList

  vListInsertEnd (Thumb, 28 bytes, Stack size 0 bytes, list.o(i.vListInsertEnd))
  [Called By]

  - >> xTaskResumeAll
  - >> vTaskIncrementTick
  - >> xTaskGenericCreate

  vPortEnterCritical (Thumb, 12 bytes, Stack size 0 bytes, port_m0.o(i.vPortEnterCritical))
  [Called By]

  - >> xTaskResumeAll
  - >> prvCheckTasksWaitingTermination
  - >> xTaskGenericCreate

  vPortExitCritical (Thumb, 14 bytes, Stack size 0 bytes, port_m0.o(i.vPortExitCritical))
  [Called By]

  - >> xTaskResumeAll
  - >> prvCheckTasksWaitingTermination
  - >> xTaskGenericCreate

  vPortFree (Thumb, 22 bytes, Stack size 8 bytes, heap_3.o(i.vPortFree))
  [Stack]

  - Max Depth = 56
  - Call Chain = vPortFree ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> xTaskResumeAll
  - >> vTaskSuspendAll
  - >> free
  [Called By]
  - >> prvCheckTasksWaitingTermination
  - >> xTaskGenericCreate

  vPortYieldFromISR (Thumb, 10 bytes, Stack size 0 bytes, port_m0.o(i.vPortYieldFromISR))
  [Called By]

  - >> xTaskResumeAll
  - >> prvIdleTask
  - >> xTaskGenericCreate
  - >> vTaskDelay

  vTaskDelay (Thumb, 44 bytes, Stack size 8 bytes, tasks.o(i.vTaskDelay))
  [Stack]

  - Max Depth = 56
  - Call Chain = vTaskDelay ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vPortYieldFromISR
  - >> uxListRemove
  - >> xTaskResumeAll
  - >> vTaskSuspendAll
  - >> prvAddCurrentTaskToDelayedList
  [Called By]
  - >> vLEDTask2
  - >> vLEDTask1
  - >> vLEDTask0

  vTaskIncrementTick (Thumb, 166 bytes, Stack size 24 bytes, tasks.o(i.vTaskIncrementTick))
  [Stack]

  - Max Depth = 24
  - Call Chain = vTaskIncrementTick
  [Calls]
  - >> vListInsertEnd
  - >> uxListRemove
  [Called By]
  - >> xTaskResumeAll
  - >> xPortSysTickHandler

  vTaskStartScheduler (Thumb, 52 bytes, Stack size 24 bytes, tasks.o(i.vTaskStartScheduler))
  [Stack]

  - Max Depth = 128
  - Call Chain = vTaskStartScheduler ⇒ xTaskGenericCreate ⇒ pvPortMalloc ⇒ malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> xPortStartScheduler
  - >> xTaskGenericCreate
  [Called By]
  - >> main

  vTaskSuspendAll (Thumb, 10 bytes, Stack size 0 bytes, tasks.o(i.vTaskSuspendAll))
  [Called By]

  - >> vPortFree
  - >> pvPortMalloc
  - >> prvCheckTasksWaitingTermination
  - >> vTaskDelay

  vTaskSwitchContext (Thumb, 124 bytes, Stack size 16 bytes, tasks.o(i.vTaskSwitchContext))
  [Stack]

  - Max Depth = 24
  - Call Chain = vTaskSwitchContext ⇒ memcmp
  [Calls]
  - >> vApplicationStackOverflowHook
  - >> memcmp
  [Called By]
  - >> xPortPendSVHandler

  xPortStartScheduler (Thumb, 58 bytes, Stack size 8 bytes, port_m0.o(i.xPortStartScheduler))
  [Stack]

  - Max Depth = 8
  - Call Chain = xPortStartScheduler
  [Calls]
  - >> vPortStartFirstTask
  - >> __aeabi_uidivmod
  [Called By]
  - >> vTaskStartScheduler

  xPortSysTickHandler (Thumb, 20 bytes, Stack size 8 bytes, port_m0.o(i.xPortSysTickHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = xPortSysTickHandler ⇒ vTaskIncrementTick
  [Calls]
  - >> vTaskIncrementTick
  [Address Reference Count : 1]
  - keil_freertos_startup_lpc8xx.o(RESET)

  xTaskGenericCreate (Thumb, 358 bytes, Stack size 40 bytes, tasks.o(i.xTaskGenericCreate))
  [Stack]

  - Max Depth = 104
  - Call Chain = xTaskGenericCreate ⇒ pvPortMalloc ⇒ malloc ⇒ __Heap_Full ⇒ __Heap_ProvideMemory ⇒ free
  [Calls]
  - >> vPortYieldFromISR
  - >> vPortFree
  - >> vPortExitCritical
  - >> vPortEnterCritical
  - >> vListInsertEnd
  - >> vListInitialiseItem
  - >> vListInitialise
  - >> pxPortInitialiseStack
  - >> pvPortMalloc
  - >> strncpy
  - >> __aeabi_memset
  [Called By]
  - >> vTaskStartScheduler
  - >> main

  xTaskResumeAll (Thumb, 162 bytes, Stack size 24 bytes, tasks.o(i.xTaskResumeAll))
  [Stack]

  - Max Depth = 48
  - Call Chain = xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vPortYieldFromISR
  - >> vPortExitCritical
  - >> vPortEnterCritical
  - >> vListInsertEnd
  - >> uxListRemove
  - >> vTaskIncrementTick
  [Called By]
  - >> vPortFree
  - >> pvPortMalloc
  - >> prvCheckTasksWaitingTermination
  - >> vTaskDelay

  ### Local Symbols

  vLEDTask0 (Thumb, 26 bytes, Stack size 0 bytes, freertos_blinky.o(i.vLEDTask0))
  [Stack]

  - Max Depth = 56
  - Call Chain = vLEDTask0 ⇒ vTaskDelay ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vTaskDelay
  - >> Board_LED_Set
  [Address Reference Count : 1]
  - freertos_blinky.o(i.main)

  vLEDTask1 (Thumb, 26 bytes, Stack size 0 bytes, freertos_blinky.o(i.vLEDTask1))
  [Stack]

  - Max Depth = 56
  - Call Chain = vLEDTask1 ⇒ vTaskDelay ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vTaskDelay
  - >> Board_LED_Set
  [Address Reference Count : 1]
  - freertos_blinky.o(i.main)

  vLEDTask2 (Thumb, 26 bytes, Stack size 0 bytes, freertos_blinky.o(i.vLEDTask2))
  [Stack]

  - Max Depth = 56
  - Call Chain = vLEDTask2 ⇒ vTaskDelay ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vTaskDelay
  - >> Board_LED_Set
  [Address Reference Count : 1]
  - freertos_blinky.o(i.main)

  prvAddCurrentTaskToDelayedList (Thumb, 46 bytes, Stack size 16 bytes, tasks.o(i.prvAddCurrentTaskToDelayedList))
  [Stack]

  - Max Depth = 24
  - Call Chain = prvAddCurrentTaskToDelayedList ⇒ vListInsert
  [Calls]
  - >> vListInsert
  [Called By]
  - >> vTaskDelay

  prvCheckTasksWaitingTermination (Thumb, 78 bytes, Stack size 16 bytes, tasks.o(i.prvCheckTasksWaitingTermination))
  [Stack]

  - Max Depth = 72
  - Call Chain = prvCheckTasksWaitingTermination ⇒ vPortFree ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vPortFree
  - >> vPortExitCritical
  - >> vPortEnterCritical
  - >> uxListRemove
  - >> xTaskResumeAll
  - >> vTaskSuspendAll
  [Called By]
  - >> prvIdleTask

  prvIdleTask (Thumb, 22 bytes, Stack size 0 bytes, tasks.o(i.prvIdleTask))
  [Stack]

  - Max Depth = 72
  - Call Chain = prvIdleTask ⇒ prvCheckTasksWaitingTermination ⇒ vPortFree ⇒ xTaskResumeAll ⇒ vTaskIncrementTick
  [Calls]
  - >> vPortYieldFromISR
  - >> vApplicationIdleHook
  - >> prvCheckTasksWaitingTermination
  [Address Reference Count : 1]
  - tasks.o(i.vTaskStartScheduler)

  Board_LED_Init (Thumb, 38 bytes, Stack size 20 bytes, board_nxp_xpresso_812.o(i.Board_LED_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = Board_LED_Init
  [Called By]
  - >> Board_Init

  Chip_Clock_EnablePeriphClock (Thumb, 14 bytes, Stack size 0 bytes, sysinit_nxp_xpresso_812.o(i.Chip_Clock_EnablePeriphClock))
  [Called By]

  - >> SystemInit

  SystemSetupClocking (Thumb, 80 bytes, Stack size 8 bytes, sysinit_nxp_xpresso_812.o(i.SystemSetupClocking))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemSetupClocking
  [Calls]
  - >> Chip_SYSCTL_PowerUp
  - >> Chip_Clock_SetSystemPllSource
  - >> Chip_Clock_SetPLLBypass
  - >> Chip_Clock_SetMainClockSource
  - >> Chip_Clock_SetCLKOUTSource
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols

  _call_atexit_fns (ARM, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit