#

##

##

    µVision3 Build Log
    Project:
    E:\XrEmbedded\Z32R\Software\Example.C1L5.340\12.1 - Timer\Timer.uv2
    Project File Date:  01/14/2009

    Output:
    Build target 'Z32R'
    assembling STM32F10x.s...
    compiling STM32_Init.c...
    compiling TFT018.c...
    compiling Timer.c...
    linking...
    Program Size: Code=3506 RO-data=5914 RW-data=8 ZI-data=1120
    ".\Output\Timer.axf" - 0 Error(s), 0 Warning(s).
    Load "E:\\XrEmbedded\\Z32R\\Software\\Example.C1L5.340\\12.1 - Timer\\Output\\Timer.AXF"
    VTarget = 3.319V
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    DLL version V4.03r, compiled Mar  9 2009 18:04:21
    Firmware: J-Link ARM V7 compiled Feb 17 2009 16:45:24
    Hardware: V7.00
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          0
    Found 2 JTAG devices, Total IRLen = 9:
     Id of device #0: 0x3BA00477
     Id of device #1: 0x16410041
    Cortex-M3 identified.
    JTAG speed: 5 kHz
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    JTAG speed: 4000 kHz
    Erase Done.
    Programming Done.
    Verify OK.
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    JTAG speed: 4000 kHz
    Application running ...