# Static Call Graph for image .\Output\CAN.axf

#<CALLGRAPH># ARM Linker, RVCT3.1 [Build 942]: Last Updated: Wed Nov 17 11:25:43 2010

### Maximum Stack Usage = 180 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__main ⇒ __rt_entry ⇒ main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - Reset_Handler
  - NMI_Handler
  - HardFault_Handler
  - MemManage_Handler
  - BusFault_Handler
  - UsageFault_Handler
  - SVC_Handler
  - DebugMon_Handler
  - PendSV_Handler
  - SysTick_Handler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMAChannel1_IRQHandler
  - DMAChannel2_IRQHandler
  - DMAChannel3_IRQHandler
  - DMAChannel4_IRQHandler
  - DMAChannel5_IRQHandler
  - DMAChannel6_IRQHandler
  - DMAChannel7_IRQHandler
  - ADC_IRQHandler
  - USB_HP_CAN_TX_IRQHandler
  - USB_LP_CAN_RX0_IRQHandler
  - CAN_RX1_IRQHandler
  - CAN_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - USBWakeUp_IRQHandler
  - __main
  - _sputc
  - _printf_outstr_char
  - _printf_input_char
  - __I_use_semihosting

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Stack]

  - Max Depth = 180 + Unknown Stack Size
  - Call Chain = __main ⇒ __rt_entry ⇒ main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __ARM_argv_veneer (Thumb, 4 bytes, Stack size 0 bytes, lib_init.o(.emb_text))
  [Calls]

  - >> __ARM_get_argv
  [Called By]
  - >> __rt_lib_init

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, stm32f10x.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  stm32_EfiSetup (Thumb, 8 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_ClockSetup (Thumb, 52 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_NvicSetup (Thumb, 4 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_IwdgSetup (Thumb, 32 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_SysTickSetup (Thumb, 28 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_RtcSetup (Thumb, 182 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_TimerSetup (Thumb, 102 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_GpioSetup (Thumb, 84 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_UsartSetup (Thumb, 160 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_ExtiSetup (Thumb, 34 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_AfRemapSetup (Thumb, 24 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_TamperSetup (Thumb, 102 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_Init (Thumb, 24 bytes, Stack size 4 bytes, stm32_init.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = stm32_Init
  [Calls]
  - >> stm32_UsartSetup
  - >> stm32_GpioSetup
  - >> stm32_TimerSetup
  - >> stm32_ClockSetup
  - >> stm32_EfiSetup
  [Called By]
  - >> main

  stm32_GetPCLK1 (Thumb, 4 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> CAN_setup

  LCD_Bus_Initial (Thumb, 114 bytes, Stack size 4 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_Bus_Initial
  [Calls]
  - >> delay
  [Called By]
  - >> LCD_Init

  LCD_Bus_Write_Byte (Thumb, 48 bytes, Stack size 4 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = LCD_Bus_Write_Byte
  [Calls]
  - >> delay
  [Called By]
  - >> LCD_BMP
  - >> PutGB1616
  - >> LCD_PutChar8x8
  - >> LCD_PutChar8x16
  - >> LCD_SetPixel
  - >> LCD_Rectangle
  - >> LCD_Reg_Set
  - >> LCD_Data
  - >> LCD_Inst
  - >> LCD_Bus_Write_Data

  LCD_Bus_Write_Data (Thumb, 18 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_Bus_Write_Byte

  LCD_Bus_Read_Byte (Thumb, 52 bytes, Stack size 4 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> delay

  LCD_Inst (Thumb, 56 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_Bus_Write_Byte

  LCD_Data (Thumb, 56 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_Bus_Write_Byte

  LCD_Reg_Set (Thumb, 76 bytes, Stack size 12 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_SetArea
  - >> LCD_Init

  LCD_Init (Thumb, 208 bytes, Stack size 4 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = LCD_Init ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Reg_Set
  - >> LCD_Bus_Initial
  [Called By]
  - >> main

  LCD_SetArea (Thumb, 60 bytes, Stack size 20 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Reg_Set
  [Called By]
  - >> LCD_BMP
  - >> PutGB1616
  - >> LCD_PutChar8x8
  - >> LCD_PutChar8x16
  - >> LCD_SetPixel
  - >> LCD_Rectangle

  LCD_Rectangle (Thumb, 124 bytes, Stack size 32 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = LCD_Rectangle ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> main
  - >> LCD_Clear_Screen

  LCD_Clear_Screen (Thumb, 20 bytes, Stack size 12 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = LCD_Clear_Screen ⇒ LCD_Rectangle ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Rectangle
  [Called By]
  - >> main

  LCD_SetPixel (Thumb, 78 bytes, Stack size 16 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte

  LCD_PutChar8x16 (Thumb, 188 bytes, Stack size 36 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_PutChar8x16 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_PutChar

  LCD_PutChar8x8 (Thumb, 170 bytes, Stack size 36 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_PutChar

  PutGB1616 (Thumb, 228 bytes, Stack size 36 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = PutGB1616 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_PutString

  LCD_PutChar (Thumb, 60 bytes, Stack size 28 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_PutChar8x8
  - >> LCD_PutChar8x16
  [Called By]
  - >> LCD_PutString

  LCD_PutString (Thumb, 100 bytes, Stack size 32 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_PutChar
  - >> PutGB1616
  [Called By]
  - >> main

  LCD_BMP (Thumb, 150 bytes, Stack size 36 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte

  Delay (Thumb, 10 bytes, Stack size 0 bytes, candemo.o(.text))
  [Called By]

  - >> main

  adc_Init (Thumb, 118 bytes, Stack size 0 bytes, candemo.o(.text))
  [Called By]

  - >> main

  can_Init (Thumb, 24 bytes, Stack size 8 bytes, candemo.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = can_Init ⇒ CAN_wrFilter
  [Calls]
  - >> CAN_wrFilter
  - >> CAN_waitReady
  - >> CAN_start
  - >> CAN_setup
  [Called By]
  - >> main

  main (Thumb, 370 bytes, Stack size 32 bytes, candemo.o(.text))
  [Stack]

  - Max Depth = 164
  - Call Chain = main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> CAN_wrMsg
  - >> can_Init
  - >> adc_Init
  - >> Delay
  - >> LCD_PutString
  - >> LCD_Clear_Screen
  - >> LCD_Rectangle
  - >> LCD_Init
  - >> stm32_Init
  - >> __1sprintf
  [Called By]
  - >> __rt_entry

  CAN_setup (Thumb, 222 bytes, Stack size 8 bytes, can.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_setup
  [Calls]
  - >> stm32_GetPCLK1
  [Called By]
  - >> can_Init

  CAN_start (Thumb, 30 bytes, Stack size 0 bytes, can.o(.text))
  [Called By]

  - >> can_Init

  CAN_testmode (Thumb, 36 bytes, Stack size 0 bytes, can.o(.text), UNUSED)

  CAN_waitReady (Thumb, 22 bytes, Stack size 0 bytes, can.o(.text))
  [Called By]

  - >> can_Init

  CAN_wrMsg (Thumb, 202 bytes, Stack size 0 bytes, can.o(.text))
  [Called By]

  - >> main

  CAN_rdMsg (Thumb, 180 bytes, Stack size 0 bytes, can.o(.text))
  [Called By]

  - >> USB_LP_CAN_RX0_IRQHandler

  CAN_wrFilter (Thumb, 208 bytes, Stack size 12 bytes, can.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = CAN_wrFilter
  [Called By]
  - >> can_Init

  USB_HP_CAN_TX_IRQHandler (Thumb, 52 bytes, Stack size 0 bytes, can.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 28 bytes, Stack size 4 bytes, can.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = USB_LP_CAN_RX0_IRQHandler
  [Calls]
  - >> CAN_rdMsg
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  __printf (Thumb, 734 bytes, Stack size 56 bytes, __printf.o(.text), UNUSED)
  [Calls]

  - >> _printf_longlong_hex
  - >> _printf_wctomb (Weak Reference)
  - >> _printf_wc (Weak Reference)
  - >> _printf_str (Weak Reference)
  - >> _printf_mbtowc (Weak Reference)
  - >> _printf_longlong_oct (Weak Reference)
  - >> _printf_longlong_dec (Weak Reference)
  - >> _printf_int_dec (Weak Reference)
  - >> _printf_fp_hex (Weak Reference)
  - >> _printf_fp_dec (Weak Reference)
  - >> _printf_charcount (Weak Reference)
  [Called By]
  - >> _printf_char_common

  _printf_return_value (Thumb, 2 bytes, Stack size 0 bytes, __printf.o(.text), UNUSED)

  _printf_percent (Thumb, 2 bytes, Stack size 0 bytes, __printf.o(.text), UNUSED)

  _printf_sizespec (Thumb, 2 bytes, Stack size 0 bytes, __printf.o(.text), UNUSED)

  _printf_pre_padding (Thumb, 42 bytes, Stack size 16 bytes, _printf_pad.o(.text), UNUSED)
  [Called By]

  - >> _printf_int_common

  _printf_post_padding (Thumb, 34 bytes, Stack size 16 bytes, _printf_pad.o(.text), UNUSED)
  [Called By]

  - >> _printf_int_common

  _printf_longlong_hex (Thumb, 188 bytes, Stack size 72 bytes, _printf_longlong_hex.o(.text), UNUSED)
  [Calls]

  - >> _printf_int_common
  - >> _printf_truncate_unsigned (Weak Reference)
  [Called By]
  - >> __printf

  __0sprintf (Thumb, 38 bytes, Stack size 32 bytes, __0sprintf.o(.text), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_char_common

  __1sprintf (Thumb, 0 bytes, Stack size 32 bytes, __0sprintf.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = __1sprintf
  [Called By]
  - >> main

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, stkheap2.o(.text), UNUSED)

  __rt_stackheap_init (Thumb, 24 bytes, Stack size 16 bytes, stkheap2.o(.text))
  [Stack]

  - Max Depth = 24 + Unknown Stack Size
  - Call Chain = __rt_stackheap_init ⇒ __user_setup_stackheap
  [Calls]
  - >> __rt_stackheap_storage
  - >> __user_setup_stackheap
  [Called By]
  - >> __rt_entry

  __rt_heap_extend (Thumb, 12 bytes, Stack size 8 bytes, stkheap2.o(.text), UNUSED)
  [Calls]

  - >> __user_heap_extend (Weak Reference)

  __rt_entry (Thumb, 36 bytes, Stack size 16 bytes, kernel.o(.text))
  [Stack]

  - Max Depth = 180 + Unknown Stack Size
  - Call Chain = __rt_entry ⇒ main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> main
  - >> _platform_post_lib_init
  - >> _platform_post_stackheap_init
  - >> __rt_lib_init
  - >> exit
  - >> __rt_stackheap_init
  [Called By]
  - >> __scatterload_rt2
  - >> __main

  __rt_exit (Thumb, 18 bytes, Stack size 8 bytes, kernel.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __rt_exit ⇒ __rt_lib_shutdown
  [Calls]
  - >> __rt_lib_shutdown
  [Called By]
  - >> exit

  __rt_abort (Thumb, 8 bytes, Stack size 0 bytes, kernel.o(.text), UNUSED)
  [Calls]

  - >> _sys_exit

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_stackheap_init

  __rt_stackheap_storage (Thumb, 6 bytes, Stack size 0 bytes, rt_stackheap_storage_intlibspace.o(.text))
  [Called By]

  - >> __rt_stackheap_init

  _printf_int_common (Thumb, 162 bytes, Stack size 32 bytes, _printf_intcommon.o(.text), UNUSED)
  [Calls]

  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_longlong_hex

  _printf_char_common (Thumb, 42 bytes, Stack size 88 bytes, _printf_char_common.o(.text), UNUSED)
  [Calls]

  - >> __printf
  [Called By]
  - >> __0sprintf

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __0sprintf
  [Address Reference Count : 1]
  - __0sprintf.o(.text)

  _sys_exit (Thumb, 16 bytes, Stack size 0 bytes, sys_exit.o(.text), UNUSED)
  [Called By]

  - >> __rt_abort

  __user_libspace (Thumb, 4 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _printf_outstr_char (Thumb, 26 bytes, Stack size 16 bytes, _printf_outstr_char.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_outstr_char
  [Address Reference Count : 1]
  - _printf_char_common.o(.text)

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_input_char.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = exit ⇒ __rt_exit ⇒ __rt_lib_shutdown
  [Calls]
  - >> _call_atexit_fns (Weak Reference)
  - >> __rt_exit
  [Called By]
  - >> __rt_entry

  __rt_lib_init (Thumb, 174 bytes, Stack size 40 bytes, lib_init.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> _fp_init
  - >> __rt_locale
  - >> _signal_init (Weak Reference)
  - >> _rand_init (Weak Reference)
  - >> _initio (Weak Reference)
  - >> _init_user_alloc (Weak Reference)
  - >> _init_alloc (Weak Reference)
  - >> _getenv_init (Weak Reference)
  - >> _get_lc_time (Weak Reference)
  - >> _get_lc_numeric (Weak Reference)
  - >> _get_lc_monetary (Weak Reference)
  - >> _get_lc_ctype (Weak Reference)
  - >> _get_lc_collate (Weak Reference)
  - >> _fp_trap_init (Weak Reference)
  - >> _clock_init (Weak Reference)
  - >> _atexit_init (Weak Reference)
  - >> __cpp_initialize__aeabi_ (Weak Reference)
  - >> __alloca_initialize (Weak Reference)
  - >> __Heap_DescSize (Weak Reference)
  - >> __ARM_exceptions_init (Weak Reference)
  - >> __ARM_argv_veneer
  [Called By]
  - >> __rt_entry

  __rt_lib_shutdown (Thumb, 18 bytes, Stack size 8 bytes, lib_init.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __rt_lib_shutdown
  [Calls]
  - >> _terminateio (Weak Reference)
  - >> _terminate_user_alloc (Weak Reference)
  - >> __cxa_finalize (Weak Reference)
  [Called By]
  - >> __rt_exit

  _platform_post_stackheap_init (Thumb, 10 bytes, Stack size 0 bytes, boardinit2.o(.text))
  [Called By]

  - >> __rt_entry

  _platform_post_lib_init (Thumb, 8 bytes, Stack size 8 bytes, boardinit3.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _platform_post_lib_init
  [Called By]
  - >> __rt_entry

  __I_use_semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text))
  [Address Reference Count : 1]

  - sys_exit.o(.text)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __rt_locale (Thumb, 6 bytes, Stack size 0 bytes, rt_locale_intlibspace.o(.text))
  [Called By]

  - >> __rt_lib_init

  __ARM_get_argv (Thumb, 2 bytes, Stack size 0 bytes, no_argv.o(.text))
  [Called By]

  - >> __ARM_argv_veneer

  __rt_fp_status_addr (Thumb, 6 bytes, Stack size 0 bytes, rt_fp_status_addr_intlibspace.o(.text))
  [Called By]

  - >> _fp_init

  _fp_init (Thumb, 14 bytes, Stack size 8 bytes, fpinit.o(x$fpl$fpinit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _fp_init
  [Calls]
  - >> __rt_fp_status_addr
  [Called By]
  - >> __rt_lib_init

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  ### Local Symbols

  delay (Thumb, 14 bytes, Stack size 0 bytes, tft018.o(.text))
  [Called By]

  - >> LCD_Bus_Read_Byte
  - >> LCD_Bus_Write_Byte
  - >> LCD_Bus_Initial

  ### Undefined Global Symbols

  __ARM_exceptions_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  __Heap_DescSize (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  __alloca_initialize (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  __cpp_initialize__aeabi_ (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  __cxa_finalize (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_shutdown (Weak Reference)

  __user_heap_extend (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __rt_heap_extend (Weak Reference)

  _atexit_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _call_atexit_fns (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> exit (Weak Reference)

  _clock_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _fp_trap_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _get_lc_collate (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _get_lc_ctype (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _get_lc_monetary (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _get_lc_numeric (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _get_lc_time (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _getenv_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _init_alloc (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _init_user_alloc (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _initio (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _printf_charcount (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_fp_dec (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_fp_hex (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_int_dec (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_longlong_dec (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_longlong_oct (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_mbtowc (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_str (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_truncate_unsigned (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> _printf_longlong_hex (Weak Reference)

  _printf_wc (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _printf_wctomb (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED, UNUSED)
  [Called By]

  - >> __printf (Weak Reference)

  _rand_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _signal_init (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_init (Weak Reference)

  _terminate_user_alloc (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_shutdown (Weak Reference)

  _terminateio (Unknown, 0 bytes, Stack size 0 bytes, UNDEFINED)
  [Called By]

  - >> __rt_lib_shutdown (Weak Reference)