# Static Call Graph for image .\Output\Timer.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 524]: Last Updated: Thu May 28 08:24:37 2009

### Maximum Stack Usage = 160 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - Reset_Handler
  - NMI_Handler
  - HardFault_Handler
  - MemManage_Handler
  - BusFault_Handler
  - UsageFault_Handler
  - SVC_Handler
  - DebugMon_Handler
  - PendSV_Handler
  - SysTick_Handler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMAChannel1_IRQHandler
  - DMAChannel2_IRQHandler
  - DMAChannel3_IRQHandler
  - DMAChannel4_IRQHandler
  - DMAChannel5_IRQHandler
  - DMAChannel6_IRQHandler
  - DMAChannel7_IRQHandler
  - ADC_IRQHandler
  - USB_HP_CAN_TX_IRQHandler
  - USB_LP_CAN_RX0_IRQHandler
  - CAN_RX1_IRQHandler
  - CAN_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - USBWakeUp_IRQHandler
  - __main
  - __I$use$semihosting

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - stm32f10x.o(RESET)

  CAN_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  CAN_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  DMAChannel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, stm32f10x.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, stm32f10x.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  stm32_EfiSetup (Thumb, 8 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_ClockSetup (Thumb, 52 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_NvicSetup (Thumb, 4 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_IwdgSetup (Thumb, 32 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_SysTickSetup (Thumb, 28 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_RtcSetup (Thumb, 182 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_TimerSetup (Thumb, 190 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_GpioSetup (Thumb, 84 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_UsartSetup (Thumb, 158 bytes, Stack size 0 bytes, stm32_init.o(.text))
  [Called By]

  - >> stm32_Init

  stm32_ExtiSetup (Thumb, 34 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_AfRemapSetup (Thumb, 24 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_TamperSetup (Thumb, 102 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  stm32_Init (Thumb, 24 bytes, Stack size 4 bytes, stm32_init.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = stm32_Init
  [Calls]
  - >> stm32_UsartSetup
  - >> stm32_GpioSetup
  - >> stm32_TimerSetup
  - >> stm32_ClockSetup
  - >> stm32_EfiSetup
  [Called By]
  - >> main

  stm32_GetPCLK1 (Thumb, 4 bytes, Stack size 0 bytes, stm32_init.o(.text), UNUSED)

  LCD_Bus_Initial (Thumb, 114 bytes, Stack size 8 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Bus_Initial
  [Calls]
  - >> delay
  [Called By]
  - >> LCD_Init

  LCD_Bus_Write_Byte (Thumb, 48 bytes, Stack size 8 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = LCD_Bus_Write_Byte
  [Calls]
  - >> delay
  [Called By]
  - >> LCD_BMP
  - >> PutGB1616
  - >> LCD_PutChar8x8
  - >> LCD_PutChar8x16
  - >> LCD_SetPixel
  - >> LCD_Rectangle
  - >> LCD_Reg_Set
  - >> LCD_Data
  - >> LCD_Inst
  - >> LCD_Bus_Write_Data

  LCD_Bus_Write_Data (Thumb, 18 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_Bus_Write_Byte

  LCD_Bus_Read_Byte (Thumb, 52 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> delay

  LCD_Inst (Thumb, 56 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_Bus_Write_Byte

  LCD_Data (Thumb, 56 bytes, Stack size 8 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_Bus_Write_Byte

  LCD_Reg_Set (Thumb, 76 bytes, Stack size 16 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_SetArea
  - >> LCD_Init

  LCD_Init (Thumb, 208 bytes, Stack size 8 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_Init ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Reg_Set
  - >> LCD_Bus_Initial
  [Called By]
  - >> main

  LCD_SetArea (Thumb, 64 bytes, Stack size 24 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Reg_Set
  [Called By]
  - >> LCD_BMP
  - >> PutGB1616
  - >> LCD_PutChar8x8
  - >> LCD_PutChar8x16
  - >> LCD_SetPixel
  - >> LCD_Rectangle

  LCD_Rectangle (Thumb, 124 bytes, Stack size 32 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = LCD_Rectangle ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_Clear_Screen

  LCD_Clear_Screen (Thumb, 20 bytes, Stack size 16 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = LCD_Clear_Screen ⇒ LCD_Rectangle ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_Rectangle
  [Called By]
  - >> main

  LCD_SetPixel (Thumb, 78 bytes, Stack size 16 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte

  LCD_PutChar8x16 (Thumb, 188 bytes, Stack size 40 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_PutChar8x16 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_PutChar

  LCD_PutChar8x8 (Thumb, 170 bytes, Stack size 40 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_PutChar

  PutGB1616 (Thumb, 232 bytes, Stack size 56 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = PutGB1616 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte
  [Called By]
  - >> LCD_PutString

  LCD_PutChar (Thumb, 60 bytes, Stack size 32 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_PutChar8x8
  - >> LCD_PutChar8x16
  [Called By]
  - >> LCD_PutString

  LCD_PutString (Thumb, 100 bytes, Stack size 32 bytes, tft018.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_PutChar
  - >> PutGB1616
  [Called By]
  - >> main

  LCD_BMP (Thumb, 150 bytes, Stack size 40 bytes, tft018.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetArea
  - >> LCD_Bus_Write_Byte

  TIM1_UP_IRQHandler (Thumb, 72 bytes, Stack size 0 bytes, timer.o(.text))
  [Address Reference Count : 1]

  - stm32f10x.o(RESET)

  main (Thumb, 130 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = main ⇒ LCD_PutString ⇒ LCD_PutChar ⇒ LCD_PutChar8x8 ⇒ LCD_SetArea ⇒ LCD_Reg_Set ⇒ LCD_Bus_Write_Byte
  [Calls]
  - >> LCD_PutString
  - >> LCD_Clear_Screen
  - >> LCD_Init
  - >> stm32_Init
  [Called By]
  - >> __rt_entry_main

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 16 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text))
  [Address Reference Count : 1]

  - sys_exit.o(.text)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  ### Local Symbols

  delay (Thumb, 14 bytes, Stack size 0 bytes, tft018.o(.text))
  [Called By]

  - >> LCD_Bus_Read_Byte
  - >> LCD_Bus_Write_Byte
  - >> LCD_Bus_Initial

  ### Undefined Global Symbols