#

##

##

    礦ision3 Build Log
    Project:
    E:\ZERO\DevKit\Lily\公司文件\产品资料\ARM7开发板\STM32开发板\Example\Example.C1L5-JLINK.340\Example.C1L5.340\9.3 - SD_RTL_xr\SD_RTL.uv2
    Project File Date:  11/10/2010

    Output:
    Load "E:\\ZERO\\DevKit\\Lily\\公司文件\\产品资料\\ARM7开发板\\STM32开发板\\Example\\Example.C1L5-JLINK.340\\Example.C1L5.340\\9.3 - SD_RTL_xr\\Output\\SD_RTL.AXF"
    VTarget = 3.300V
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    ***JLink Warning: Could not set S_RESET_ST
    DLL version V4.20h, compiled Oct  5 2010 19:11:41
    Firmware: J-Link ARM-OB STM32 compiled Dec 15 2010 11:30:03
    Hardware: V7.00
    Hardware-Breakpoints: 6
    Software-Breakpoints: 2048
    Watchpoints:          0
    Found 2 JTAG devices, Total IRLen = 9:
     Id of device #0: 0x3BA00477
     Id of device #1: 0x16410041
    Cortex-M3 identified.
    JTAG speed: 5 kHz
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    JTAG speed: 1000 kHz
    Erase Done.
    Programming Done.
    Verify OK.
    Info: TotalIRLen = 9, IRPrint = 0x0011
    Info: Found Cortex-M3 r1p1, Little endian.
    Info: TPIU fitted.
    Info:   FPUnit: 6 code (BP) slots and 2 literal slots
    JTAG speed: 1000 kHz
    Application running ...