# Static Call Graph for image .\Obj\I2C.axf

#<CALLGRAPH># ARM Linker, RVCT4.0 [Build 524]: Last Updated: Thu Oct 22 15:23:30 2009

### Maximum Stack Usage = 200 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ I2C_Test ⇒ I2C_WriteS_24C ⇒ I2C_PageWrite_24C ⇒ I2C_CheckEvent

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - Reset_Handler
  - NMI_Handler
  - HardFault_Handler
  - MemManage_Handler
  - BusFault_Handler
  - UsageFault_Handler
  - SVC_Handler
  - DebugMon_Handler
  - PendSV_Handler
  - SysTick_Handler
  - WWDG_IRQHandler
  - PVD_IRQHandler
  - TAMPER_IRQHandler
  - RTC_IRQHandler
  - FLASH_IRQHandler
  - RCC_IRQHandler
  - EXTI0_IRQHandler
  - EXTI1_IRQHandler
  - EXTI2_IRQHandler
  - EXTI3_IRQHandler
  - EXTI4_IRQHandler
  - DMA1_Channel1_IRQHandler
  - DMA1_Channel2_IRQHandler
  - DMA1_Channel3_IRQHandler
  - DMA1_Channel4_IRQHandler
  - DMA1_Channel5_IRQHandler
  - DMA1_Channel6_IRQHandler
  - DMA1_Channel7_IRQHandler
  - ADC1_2_IRQHandler
  - CAN1_TX_IRQHandler
  - CAN1_RX0_IRQHandler
  - CAN1_RX1_IRQHandler
  - CAN1_SCE_IRQHandler
  - EXTI9_5_IRQHandler
  - TIM1_BRK_IRQHandler
  - TIM1_UP_IRQHandler
  - TIM1_TRG_COM_IRQHandler
  - TIM1_CC_IRQHandler
  - TIM2_IRQHandler
  - TIM3_IRQHandler
  - TIM4_IRQHandler
  - I2C1_EV_IRQHandler
  - I2C1_ER_IRQHandler
  - I2C2_EV_IRQHandler
  - I2C2_ER_IRQHandler
  - SPI1_IRQHandler
  - SPI2_IRQHandler
  - USART1_IRQHandler
  - USART2_IRQHandler
  - USART3_IRQHandler
  - EXTI15_10_IRQHandler
  - RTCAlarm_IRQHandler
  - OTG_FS_WKUP_IRQHandler
  - TIM5_IRQHandler
  - SPI3_IRQHandler
  - UART4_IRQHandler
  - UART5_IRQHandler
  - TIM6_IRQHandler
  - TIM7_IRQHandler
  - DMA2_Channel1_IRQHandler
  - DMA2_Channel2_IRQHandler
  - DMA2_Channel3_IRQHandler
  - DMA2_Channel4_IRQHandler
  - DMA2_Channel5_IRQHandler
  - ETH_IRQHandler
  - ETH_WKUP_IRQHandler
  - CAN2_TX_IRQHandler
  - CAN2_RX0_IRQHandler
  - CAN2_RX1_IRQHandler
  - CAN2_SCE_IRQHandler
  - OTG_FS_IRQHandler
  - __main
  - __I$use$semihosting

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 100 bytes, Stack size unknown bytes, __dclz77c.o(!!dclz77c), UNUSED)

  __decompress2 (Thumb, 0 bytes, Stack size unknown bytes, __dclz77c.o(!!dclz77c), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ I2C_Test ⇒ I2C_WriteS_24C ⇒ I2C_PageWrite_24C ⇒ I2C_CheckEvent
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  rd_reg (Thumb, 110 bytes, Stack size 8 bytes, glcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = rd_reg
  [Calls]
  - >> wr_cmd
  [Called By]
  - >> GLCD_init

  GLCD_init (Thumb, 1044 bytes, Stack size 8 bytes, glcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GLCD_init ⇒ wr_reg
  [Calls]
  - >> wr_reg
  - >> rd_reg
  - >> delay
  [Called By]
  - >> InitDis

  GLCD_putPixel (Thumb, 34 bytes, Stack size 16 bytes, glcd.o(.text), UNUSED)
  [Calls]

  - >> wr_reg

  GLCD_setTextColor (Thumb, 6 bytes, Stack size 0 bytes, glcd.o(.text))
  [Called By]

  - >> InitDis

  GLCD_setBackColor (Thumb, 8 bytes, Stack size 0 bytes, glcd.o(.text), UNUSED)

  GLCD_clear (Thumb, 58 bytes, Stack size 16 bytes, glcd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = GLCD_clear ⇒ wr_reg
  [Calls]
  - >> wr_reg
  - >> wr_dat
  - >> wr_cmd
  [Called By]
  - >> InitDis

  GLCD_drawChar (Thumb, 134 bytes, Stack size 32 bytes, glcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = GLCD_drawChar ⇒ wr_reg
  [Calls]
  - >> wr_reg
  - >> wr_dat
  - >> wr_cmd
  [Called By]
  - >> GLCD_displayChar

  GLCD_displayChar (Thumb, 34 bytes, Stack size 16 bytes, glcd.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = GLCD_displayChar ⇒ GLCD_drawChar ⇒ wr_reg
  [Calls]
  - >> GLCD_drawChar
  [Called By]
  - >> GLCD_displayStringLn

  GLCD_displayStringLn (Thumb, 60 bytes, Stack size 24 bytes, glcd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = GLCD_displayStringLn ⇒ GLCD_displayChar ⇒ GLCD_drawChar ⇒ wr_reg
  [Calls]
  - >> GLCD_displayChar
  [Called By]
  - >> InitDis
  - >> GLCD_clearLn

  GLCD_clearLn (Thumb, 14 bytes, Stack size 8 bytes, glcd.o(.text), UNUSED)
  [Calls]

  - >> GLCD_displayStringLn

  GLCD_bitmap (Thumb, 122 bytes, Stack size 40 bytes, glcd.o(.text), UNUSED)
  [Calls]

  - >> wr_reg
  - >> wr_dat
  - >> wr_cmd

  GLCD_Test (Thumb, 168 bytes, Stack size 16 bytes, glcd.o(.text), UNUSED)
  [Calls]

  - >> wr_reg
  - >> wr_dat
  - >> wr_cmd

  GPIO_Configuration (Thumb, 80 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  [Called By]
  - >> Init_All_Periph

  NVIC_Configuration (Thumb, 22 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = NVIC_Configuration
  [Calls]
  - >> NVIC_SetVectorTable
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> Init_All_Periph

  RCC_Configuration (Thumb, 34 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_Configuration ⇒ SystemInit ⇒ SetSysClock
  [Calls]
  - >> SystemInit
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHBPeriphClockCmd
  [Called By]
  - >> Init_All_Periph

  InitDis (Thumb, 46 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = InitDis ⇒ GLCD_displayStringLn ⇒ GLCD_displayChar ⇒ GLCD_drawChar ⇒ wr_reg
  [Calls]
  - >> GLCD_displayStringLn
  - >> GLCD_clear
  - >> GLCD_setTextColor
  - >> GLCD_init
  [Called By]
  - >> Init_All_Periph

  Init_All_Periph (Thumb, 24 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 108 + Unknown Stack Size
  - Call Chain = Init_All_Periph ⇒ I2C_Configuration ⇒ I2C_Init ⇒ RCC_GetClocksFreq ⇒ __user_setup_stackheap
  [Calls]
  - >> I2C_Configuration
  - >> InitDis
  - >> RCC_Configuration
  - >> NVIC_Configuration
  - >> GPIO_Configuration
  [Called By]
  - >> main

  main (Thumb, 14 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = main ⇒ I2C_Test ⇒ I2C_WriteS_24C ⇒ I2C_PageWrite_24C ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_Test
  - >> Init_All_Periph
  [Called By]
  - >> __rt_entry_main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C_Configuration (Thumb, 110 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 100 + Unknown Stack Size
  - Call Chain = I2C_Configuration ⇒ I2C_Init ⇒ RCC_GetClocksFreq ⇒ __user_setup_stackheap
  [Calls]
  - >> I2C_Init
  - >> I2C_DeInit
  - >> I2C_Cmd
  - >> I2C_AcknowledgeConfig
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> Init_All_Periph

  I2C_ReadS_24C (Thumb, 152 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_ReadS_24C ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_Send7bitAddress
  - >> I2C_ReceiveData
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> I2C_Test

  I2C_Standby_24C (Thumb, 64 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_Standby_24C
  [Calls]
  - >> I2C_Send7bitAddress
  - >> I2C_ReadRegister
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_ClearFlag
  [Called By]
  - >> I2C_WriteS_24C
  - >> I2C_ByteWrite_24C
  - >> I2C_Test

  I2C_ByteWrite_24C (Thumb, 92 bytes, Stack size 16 bytes, i2c.o(.text), UNUSED)
  [Calls]

  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_Standby_24C

  I2C_PageWrite_24C (Thumb, 120 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = I2C_PageWrite_24C ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GetFlagStatus
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  [Called By]
  - >> I2C_WriteS_24C

  I2C_WriteS_24C (Thumb, 114 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = I2C_WriteS_24C ⇒ I2C_PageWrite_24C ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_PageWrite_24C
  - >> I2C_Standby_24C
  [Called By]
  - >> I2C_Test

  I2C_Test (Thumb, 90 bytes, Stack size 136 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = I2C_Test ⇒ I2C_WriteS_24C ⇒ I2C_PageWrite_24C ⇒ I2C_CheckEvent
  [Calls]
  - >> I2C_WriteS_24C
  - >> I2C_Standby_24C
  - >> I2C_ReadS_24C
  [Called By]
  - >> main

  SystemInit (Thumb, 84 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> RCC_Configuration

  Reset_Handler (Thumb, 4 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_cl.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_cl.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_cl.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_cl.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 102 bytes, Stack size 16 bytes, misc.o(.text), UNUSED)

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_SystemLPConfig (Thumb, 38 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 268 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> I2C_Configuration
  - >> GPIO_Configuration

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 104 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 60 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  I2C_DeInit (Thumb, 50 bytes, Stack size 8 bytes, stm32f10x_i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> I2C_Configuration

  I2C_Init (Thumb, 230 bytes, Stack size 48 bytes, stm32f10x_i2c.o(.text))
  [Stack]

  - Max Depth = 76 + Unknown Stack Size
  - Call Chain = I2C_Init ⇒ RCC_GetClocksFreq ⇒ __user_setup_stackheap
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> I2C_Configuration

  I2C_StructInit (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_Configuration

  I2C_DMACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_DMALastTransferCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_GenerateSTART (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_PageWrite_24C
  - >> I2C_ByteWrite_24C
  - >> I2C_Standby_24C
  - >> I2C_ReadS_24C

  I2C_GenerateSTOP (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_PageWrite_24C
  - >> I2C_ByteWrite_24C
  - >> I2C_Standby_24C
  - >> I2C_ReadS_24C

  I2C_AcknowledgeConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_ReadS_24C
  - >> I2C_Configuration

  I2C_OwnAddress2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_DualAddressCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_GeneralCallCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_ITConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_PageWrite_24C
  - >> I2C_ByteWrite_24C

  I2C_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_ReadS_24C

  I2C_Send7bitAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_PageWrite_24C
  - >> I2C_ByteWrite_24C
  - >> I2C_Standby_24C
  - >> I2C_ReadS_24C

  I2C_ReadRegister (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_Standby_24C

  I2C_SoftwareResetCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_SMBusAlertConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_TransmitPEC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_PECPositionConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_CalculatePEC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_GetPEC (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_ARPCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_StretchClockCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_FastModeDutyCycleConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_GetLastEvent (Thumb, 26 bytes, Stack size 8 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_CheckEvent (Thumb, 38 bytes, Stack size 16 bytes, stm32f10x_i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = I2C_CheckEvent
  [Called By]
  - >> I2C_PageWrite_24C
  - >> I2C_ByteWrite_24C
  - >> I2C_ReadS_24C

  I2C_GetFlagStatus (Thumb, 42 bytes, Stack size 12 bytes, stm32f10x_i2c.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = I2C_GetFlagStatus
  [Called By]
  - >> I2C_PageWrite_24C
  - >> I2C_ReadS_24C

  I2C_ClearFlag (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text))
  [Called By]

  - >> I2C_Standby_24C

  I2C_GetITStatus (Thumb, 38 bytes, Stack size 12 bytes, stm32f10x_i2c.o(.text), UNUSED)

  I2C_ClearITPendingBit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_i2c.o(.text), UNUSED)

  RCC_DeInit (Thumb, 78 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 48 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PREDIV1Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PREDIV2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLL2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLL2Cmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLL3Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLL3Cmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_OTGFSCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_I2S2CLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_I2S3CLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 374 bytes, Stack size 20 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 28 + Unknown Stack Size
  - Call Chain = RCC_GetClocksFreq ⇒ __user_setup_stackheap
  [Calls]
  - >> RCC_ClockSecuritySystemCmd
  - >> RCC_APB1PeriphResetCmd
  - >> __user_setup_stackheap
  - >> __rt_heap_escrow$2region
  [Called By]
  - >> I2C_Init

  RCC_AHBPeriphClockCmd (Thumb, 72 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> I2C_Configuration
  - >> RCC_Configuration

  RCC_AHBPeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_GetClocksFreq
  - >> I2C_DeInit

  RCC_BackupResetCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_GetClocksFreq

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text))
  [Called By]

  - >> RCC_GetClocksFreq

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> RCC_GetClocksFreq
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 16 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text))
  [Address Reference Count : 1]

  - sys_exit.o(.text)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  wr_cmd (Thumb, 34 bytes, Stack size 0 bytes, glcd.o(i.wr_cmd))
  [Called By]

  - >> wr_reg
  - >> GLCD_Test
  - >> GLCD_bitmap
  - >> GLCD_drawChar
  - >> GLCD_clear
  - >> rd_reg

  wr_dat (Thumb, 36 bytes, Stack size 0 bytes, glcd.o(i.wr_dat))
  [Called By]

  - >> wr_reg
  - >> GLCD_Test
  - >> GLCD_bitmap
  - >> GLCD_drawChar
  - >> GLCD_clear

  wr_reg (Thumb, 32 bytes, Stack size 16 bytes, glcd.o(i.wr_reg))
  [Stack]

  - Max Depth = 16
  - Call Chain = wr_reg
  [Calls]
  - >> wr_dat
  - >> wr_cmd
  [Called By]
  - >> GLCD_Test
  - >> GLCD_bitmap
  - >> GLCD_drawChar
  - >> GLCD_clear
  - >> GLCD_putPixel
  - >> GLCD_init

  ### Local Symbols

  delay (Thumb, 14 bytes, Stack size 0 bytes, glcd.o(.text))
  [Called By]

  - >> GLCD_init

  SetSysClockTo72 (Thumb, 246 bytes, Stack size 0 bytes, system_stm32f10x.o(.text))
  [Called By]

  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SetSysClock
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  ### Undefined Global Symbols