This is an RL Flash File System file manipulation example.
You can create, read, copy, delete files from the SD/MMC 
Flash Memory Card and format the card. 

The SD_FILE program is a standalone application loaded into
on-chip flash and available for one target:

STM3210C:  Standalone application for STM3210C-EVAL Board using
           USART port as a communication interface.

           Connect a serial cable to RS232 USART port using
           HyperTerminal at 115200 baud, 8-bits, no parity,
           1 stop bit, XON/XOFF.


