/******************** (C) COPYRIGHT 2007 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V1.0
* Date               : 10/08/2007
* Description        : Description of the TIM Example5.
********************************************************************************
* THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Example description
===================

This example shows how to configure the TIM peripheral in Output Compare Timing 
mode with the corresponding Interrupt requests for each channel in order to generate
4 different time bases.

The TIMxCLK frequency is set to 36 MHz, the Prescaler is 4 so the TIM2 counter
clock is 7.2 MHz. 

The TIM2 CC1 register value is equal to 49152, 
CC1 update rate = TIM2 counter clock / CCR1_Val = 146.48 Hz,
so the TIM2 Channel 1 generates an interrupt each 6.8ms

The TIM2 CC2 register is equal to 32768, 
CC2 update rate = TIM2 counter clock / CCR2_Val = 219.7 HzHz
so the TIM2 Channel 2 generates an interrupt each 4.55ms

The TIM2 CC3 register is equal to 16384, 
CC3 update rate = TIM2 counter clock / CCR3_Val = 439.4Hz
so the TIM2 Channel 3 generates an interrupt each 2.27ms

The TIM2 CC4 register is equal to 8192, 
CC4 update rate = TIM2 counter clock / CCR4_Val =  878.9 Hz
so the TIM2 Channel 4 generates an interrupt each 1.13ms.


When the counter value reaches the Output compare registers values, the Output 
Compare interrupts are generated and, in the handler routine, 4 pins(PC.06, PC.07,
PC.08 and  PC.09) are toggled with the following frequencies: 

- PC.06: 73.24Hz (CC1)
- PC.07: 109.8Hz (CC2)
- PC.08: 219.7Hz (CC3) 
- PC.09: 439.4Hz (CC4)


Directory contents
==================
stm32F10x_conf.h  Library Configuration file
stm32F10x_it.c    Interrupt handlers
stm32F10x_it.h    Interrupt handlers header file
main.c            Main program
 

Hardware environment
====================
Connect an oscilloscope on PC.06, PC.07, PC.08 and  PC.09 to show the different
Time Base signals.
  
  
How to use it
=============
In order to make the program work, you must do the following:
- Create a project and setup all your toolchain's start-up files
- Compile the directory content files and required Library files:
  + stm32F10x_lib.c
  + stm32F10x_tim.c
  + stm32F10x_gpio.c
  + stm32F10x_rcc.c
  + stm32F10x_nvic.c
  + stm32F10x_flash.c

- Link all compiled files and load your image into either RAM or Flash
- Run the example


******************* (C) COPYRIGHT 2007 STMicroelectronics *****END OF FILE******
