/******************** (C) COPYRIGHT 2007 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V1.0
* Date               : 10/08/2007
* Description        : Description of the I2C Example4.
********************************************************************************
* THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Example description
===================
This example provides a description of how to transfer a data buffer from I2C1 to
I2C2 in 10-bit addressing mode.

After enabling the two I2C peripherals, the transfer in 10-bit addressing mode starts
after the I2C1 start condition is generated. Each time an event occurs on the master
or the slave, it is managed on I2C1 or I2C2, respectively. In this application, I2C1
Tx_Buffer is transmitted from the master (I2C1) to the slave (I2C2) and stored into
I2C2 Rx_Buffer. All transmitted and received buffers are compared to check that all
data have been correctly transferred.

The communication clock speed is set to 300KHz.


Directory contents
==================
stm32f10x_conf.h  Library Configuration file
stm32f10x_it.c    Interrupt handlers
stm32f10x_it.h    Interrupt handlers header file
main.c            Main program


Hardware environment
====================
 - Connect I2C1 SCL pin (PB.06) to I2C2 SCL pin (PB.10)
 - Connect I2C1 SDA pin (PB.07) to I2C2 SDA pin	(PB.11)
 - Check that a pull-up resistor is connected on one I2C SDA pin
 - Check that a pull-up resistor is connected on one I2C SCL pin


How to use it
=============
In order to make the program work, you must do the following :
- Create a project and setup all your toolchain's start-up files
- Compile the directory content files and required Library files:
  + stm32f10x_lib.c
  + stm32f10x_i2c.c
  + stm32f10x_rcc.c
  + stm32f10x_nvic.c
  + stm32f10x_gpio.c
  + stm32f10x_flash.c
  
- Link all compiled files and load your image into either RAM or FLASH
- Run the example


******************* (C) COPYRIGHT 2007 STMicroelectronics *****END OF FILE******
