/******************** (C) COPYRIGHT 2007 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V1.0
* Date               : 10/08/2007
* Description        : Description of the SysTick Example.
********************************************************************************
* THE PRESENT SOFTWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH SOFTWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Example description
===================

This example shows how to configure the SysTick to generate a time base equal to
1 ms. The system clock is set to 72 MHz, the SysTick is clocked by the AHB clock
(HCLK) divided by 8.

A "Delay" function is implemented based on the SysTick end-of-count event.
Four LEDs connected to the PC.06, PC.07, PC.08 and PC.09 pins are toggled with a
timing defined by the Delay function.


Directory contents
==================
stm32f10x_conf.h  Library Configuration file
stm32f10x_it.c    Interrupt handlers
stm32f10x_it.h    Header for stm32f10x_it.c
main.c            Main program
main.h            Header for main.c


Hardware environment
====================
 - Connect four leds to pins PC.06, PC.07, PC.08 and PC.09(respectively LD1, LD2, LD3  
   and LD4 on STM3210B-EVAL board).

    
How to use it
=============
In order to make the program work, you must do the following:
- Create a project and setup all your toolchain's start-up files
- Compile the directory content files and required Library files:
  + stm32f10x_lib.c
  + stm32f10x_gpio.c
  + stm32f10x_rcc.c
  + stm32f10x_systick.c
  + stm32f10x_nvic.c
  + stm32f10x_flash.c
  
- Link all compiled files and load your image into either RAM or Flash
- Run the example


******************* (C) COPYRIGHT 2007 STMicroelectronics *****END OF FILE******
