/**
  @page RTC_Tamper RTC Tamper example
  
  @verbatim
  ******************** (C) COPYRIGHT 2012 STMicroelectronics *******************
  * @file    RTC/Tamper/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-May-2012
  * @brief   Description of the RTC Tamper example.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim

@par Example Description 

This example shows how to write/read data to/from RTC Backup data registers and 
demonstrates the Tamper detection feature.

One from the following clock can be used as RTC clock source (uncomment the
corresponding define in main.c):
  - LSE oscillator clock usually delivered by a 32.768 kHz quartz.
  - LSI oscillator clock

The associated firmware performs the following:
1. It configures the Tamper pin to be falling edge, and enables the Tamper interrupt.
2. It writes the data to all RTC Backup data registers, then check whether the 
   data were correctly written. If yes, LED1 turns on, otherwise LED3 turns on.
3. On applying a low level on the RTC_AF1 pin (PC.13, connected to Tamper button), 
   the RTC backup data registers are reset and the Tamper interrupt is generated. 
   The corresponding ISR then checks whether the RTC Backup data registers are cleared.
   If yes LED2 turns ON, otherwise LED4 turns ON.
 

@par Directory contents 

  - RTC/Tamper/stm32f0xx_conf.h    Library Configuration file
  - RTC/Tamper/stm32f0xx_it.c      Interrupt handlers
  - RTC/Tamper/stm32f0xx_it.h      Interrupt handlers header file
  - RTC/Tamper/main.c              Main program
  - RTC/Tamper/main.h              Main program header file
  - RTC/Tamper/system_stm32f0xx.c  STM32F0xx system source file
  
@note The "system_stm32f0xx.c" is generated by an automatic clock configuration 
      tool and can be easily customized to meet user application requirements. 
      To select different clock setup, use the "STM32F0xx_Clock_Configuration_VX.Y.Z.xls" 
      provided with the AN4055 package available on <a href="http://www.st.com/internet/mcu/class/1734.jsp">  ST Microcontrollers </a>

         
@par Hardware and Software environment

  - This example runs on STM32F0xx Devices.
  
  - This example has been tested with STMicroelectronics STM320518-EVAL (STM32F0xx)
    evaluation board and can be easily tailored to any other supported device 
    and development board.

  - STM320518-EVAL Set-up
    - Use Tamper button.


@par How to use it ? 

In order to make the program work, you must do the following :
 - Copy all source files from this example folder to the template folder under
   Project\STM32F0xx_StdPeriph_Templates
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
