/**
  @page TIM_7_PWMOutputs TIM 7 PWM Outputs
  
  @verbatim
  ******************** (C) COPYRIGHT 2012 STMicroelectronics *******************
  * @file    TIM/7_PWMOutputs/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-May-2012
  * @brief   Description of the TIM 7PWM_Output example.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim

@par Example Description 

This example shows how to configure the TIM1 peripheral to generate 7 PWM signals 
with 4 different duty cycles (50%, 37.5%, 25% and 12.5%).

TIM1CLK = SystemCoreClock, Prescaler = 0, TIM1 counter clock = SystemCoreClock
SystemCoreClock is set to 48 MHz for STM32F0xx devices.

The objective is to generate 7 PWM signal at 17.57 KHz:
  - TIM1_Period = (SystemCoreClock / 17570) - 1
The channel 1 and channel 1N duty cycle is set to 50%
The channel 2 and channel 2N duty cycle is set to 37.5%
The channel 3 and channel 3N duty cycle is set to 25%
The channel 4 duty cycle is set to 12.5%
The Timer pulse is calculated as follows:
  - ChannelxPulse = DutyCycle * (TIM1_Period - 1) / 100

The TIM1 waveform can be displayed using an oscilloscope.


@par Directory contents 

  - TIM/7_PWMOutputs/stm32f0xx_conf.h    Library Configuration file
  - TIM/7_PWMOutputs/stm32f0xx_it.c      Interrupt handlers
  - TIM/7_PWMOutputs/stm32f0xx_it.h      Interrupt handlers header file
  - TIM/7_PWMOutputs/main.c              Main program
  - TIM/7_PWMOutputs/system_stm32f0xx.c  STM32F0xx system source file
  
@note The "system_stm32f0xx.c" is generated by an automatic clock configuration 
      tool and can be easily customized to meet user application requirements. 
      To select different clock setup, use the "STM32F0xx_Clock_Configuration_VX.Y.Z.xls" 
      provided with the AN4055 package available on <a href="http://www.st.com/internet/mcu/class/1734.jsp">  ST Microcontrollers </a>

         
@par Hardware and Software environment

  - This example runs on STM32F0xx Devices.
  
  - This example has been tested with STM32F0-Discovery board and can be easily 
    tailored to any other supported device and development board.

  - STM32F0-Discovery Set-up
    - Connect the TIM1 pins to an oscilloscope to monitor the different waveforms:
      - TIM1_CH1  pin (PA.08)
      - TIM1_CH1N pin (PA.07)
      - TIM1_CH2  pin (PA.09)
      - TIM1_CH2N pin (PB.00)
      - TIM1_CH3  pin (PA.10)
      - TIM1_CH3N pin (PB.01)
      - TIM1_CH4  pin (PA.11)


@par How to use it ? 

In order to make the program work, you must do the following :
 - Copy all source files from this example folder to the template folder under
   Project\STM32F0xx_StdPeriph_Templates
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
