/**
  @page Lib_DEBUG_Example  Lib_DEBUG Example
  
  @verbatim
  ******************** (C) COPYRIGHT 2012 STMicroelectronics *******************
  * @file    Lib_DEBUG/Lib_DEBUG_Example/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-May-2012
  * @brief   Description of the Lib_DEBUG Example.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim

@par Example  Description 

This example demonstrates how to declare a dynamic peripherals pointers used for
Debug mode.  

To use Debug mode you have to add the stm32f0xx_ip_dbg.c file to your application.
This creates a pointer to the peripheral structure in SRAM. Debugging consequently
becomes easier and all register settings can be obtained by dumping a peripheral 
variable.

When the "USE_FULL_ASSERT" label is uncommented (in stm32f0xx_conf.h file),
the assert_param macro is expanded and run-time checking is enabled in the firmware
library code. The run-time checking allows checking that all the library functions
input value lies within the parameter allowed values.

The associated program simulates wrong parameter passed to library function and the
source of the error is printed on Hyperterminal (through USART).

@note
The Debug mode increases the code size and reduces the code performance. For this
reason, it is recommended to used it only when debugging the application and to
remove it from the final application code.


@par Directory contents

  - Lib_DEBUG/Lib_DEBUG_Example/stm32f0xx_conf.h     Library Configuration file
  - Lib_DEBUG/Lib_DEBUG_Example/stm32f0xx_it.c       Interrupt handlers            
  - Lib_DEBUG/Lib_DEBUG_Example/stm32f0xx_it.h       Interrupt handlers header file
  - Lib_DEBUG/Lib_DEBUG_Example/main.c               Main program 
  - Lib_DEBUG/Lib_DEBUG_Example/main.h               Header for main.c module
  - Lib_DEBUG/Lib_DEBUG_Example/stm32f0xx_ip_dbg.c   Provides all STM32F0xx peripherals pointers initialization 
  - Lib_DEBUG/Lib_DEBUG_Example/stm32f0xx_ip_dbg.h   Header for stm32f0xx_ip_dbg.c module
  - Lib_DEBUG/Lib_DEBUG_Example/system_stm32f0xx.c   STM32F0xx system source file

@note The "system_stm32f0xx.c" is generated by an automatic clock configuration 
      tool and can be easily customized to meet user application requirements. 
      To select different clock setup, use the "STM32F0xx_Clock_Configuration_VX.Y.Z.xls" 
      provided with the AN4055 package available on <a href="http://www.st.com/internet/mcu/class/1734.jsp">  ST Microcontrollers </a>

      
@par Hardware and Software environment

  - This example runs on STM32F0xx Devices.
  
  - This example has been tested with STMicroelectronics STM320518-EVAL (STM32F0xx)
    evaluation board and can be easily tailored to any other supported device 
    and development board.

  - STM320518-EVAL Set-up
      - Connect a null-modem female/female RS232 cable between the DB9 connector CN7
        and PC serial port.

  - Hyperterminal configuration:
    - Word Length = 8 Bits
    - One Stop Bit
    - No parity
    - BaudRate = 115200 baud
    - flow control: None 


@par How to use it ? 

In order to make the program work, you must do the following :
 - Copy all source files from this example folder to the template folder under
   Project\STM32F0xx_StdPeriph_Templates
 - Open your preferred toolchain
 - Add the "stm32f0xx_ip_dbg.c" file to the project source list 
 - Rebuild all files and load your image into target memory
 - Run the example
        
 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
