/**
  @page TIM_Encoder_Mode TIM Encoder mode Description
  
  @verbatim
  ******************** (C) COPYRIGHT 2012 STMicroelectronics *******************
  * @file    TIM/Encoder_Mode/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-May-2012
  * @brief   TIM Encoder Mode Description.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim

@par Example Description 

This example shows how to configure the TIM peripheral to interface with a encoder sensor.
The TIM3 is configured in encoder mode1: Counter counts up/down on TI2 rising edge 
depending on TI1 level 

The TIM3 Autoreload value is set to 399, so the encoder round is 400 TIM counter clock. 
An update interrupt is generated each time the TIM counter reach the Autoreload value, 
in this example 400 TIM counter clock.
 

@par Directory contents 

  - TIM/TIM_Encoder_Mode/stm32f0xx_conf.h    Library Configuration file
  - TIM/TIM_Encoder_Mode/stm32f0xx_it.c      Interrupt handlers
  - TIM/TIM_Encoder_Mode/stm32f0xx_it.h      Interrupt handlers header file
  - TIM/TIM_Encoder_Mode/main.c              Main program
  - TIM/TIM_Encoder_Mode/system_stm32f0xx.c  STM32F0xx system source file
  
@note The "system_stm32f0xx.c" is generated by an automatic clock configuration 
      tool and can be easily customized to meet user application requirements. 
      To select different clock setup, use the "STM32F0xx_Clock_Configuration_VX.Y.Z.xls" 
      provided with the AN4055 package available on <a href="http://www.st.com/internet/mcu/class/1734.jsp">  ST Microcontrollers </a>
         
@par Hardware and Software environment

  - This example runs on STM32F0xx Devices.
  
  - This example has been tested with STMicroelectronics STM320518-EVAL (STM32F0xx)
    evaluation board and can be easily tailored to any other supported device 
    and development board.

@par How to use it ? 

In order to make the program work, you must do the following :
 - Copy all source files from this example folder to the template folder under
   Project\STM32F0xx_StdPeriph_Templates
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
