/**
  @page PWR_STANDBY PWR STANDBY Mode Example
  
  @verbatim
  ******************** (C) COPYRIGHT 2012 STMicroelectronics *******************
  * @file    PWR/PWR_STANDBY/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-May-2012
  * @brief   Description of the PWR STANDBY Mode Example.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim

@par PWR/PWR_STANDBY example Description 

This example shows how to enter the system to STANDBY mode and wake-up from this
mode using RTC Alarm.

In the associated software, the system clock is set to 48 MHz, the SysTick is programmed
to generate an interrupt each 250 ms. In the SysTick interrupt handler, the LED3 is
toggled, this is used to indicate whether the MCU is in STANDBY or RUN mode.

When a falling edge is detected on the PB8(pressing on user button), the RTC is 
configured to generate an Alarm event in 3 seconds then the system enters STANDBY 
mode causing the LED3 to stop toggling. 
An external RESET will wake-up the system from STANDBY. If within 3 seconds an 
external RESET is not generated, the RTC Alarm will wake-up the system. 

After wake-up from STANDBY mode, program execution restarts in the same way as after
a RESET, the LED3 is toggling again,the RTC configuration(clock source, enable, prescaler,...) 
is kept.
As result there is no need to configure the RTC.

Led LED3 is used to monitor the system state as following:
 - LED3 toggling: system in RUN mode
 - LED3 off : system in STANDBY mode

@note To measure the current consumption in STANDBY mode, please refer to 
      @subpage PWR_CurrentConsumption example.


@par Directory contents 
  - PWR/PWR_STANDBY/stm32f0xx_conf.h     Library Configuration file
  - PWR/PWR_STANDBY/stm32f0xx_it.c       Interrupt handlers
  - PWR/PWR_STANDBY/stm32f0xx_it.h       Interrupt handlers header file
  - PWR/PWR_STANDBY/main.c               Main program 
  - PWR/PWR_STANDBY/main.h               Header for main.c module
  - PWR/PWR_STANDBY/system_stm32f0xx.c   STM32F0xx system source file

@note The "system_stm32f0xx.c" is generated by an automatic clock configuration 
      tool and can be easily customized to meet user application requirements. 
      To select different clock setup, use the "STM32F0xx_Clock_Configuration_VX.Y.Z.xls" 
      provided with the AN4055 package available on <a href="http://www.st.com/internet/mcu/class/1734.jsp">  ST Microcontrollers </a>

      
@par Hardware and Software environment

  - This example runs on STM32F0xx Devices.
  
  - This example has been tested with STMicroelectronics STM320518-EVAL (STM32F0xx)
    evaluation board and can be easily tailored to any other supported device 
    and development board.

  - STM320518-EVAL Set-up
    - Use the KEY push-button connected to PB8 pin


@par How to use it ? 

In order to make the program work, you must do the following :
 - Copy all source files from this example folder to the template folder under
   Project\STM32F0xx_StdPeriph_Templates
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example
        
 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
