
T0C10 000:573 SEGGER J-Link V4.35b (beta) Log File (0001ms, 0572ms total)
T0C10 000:573 DLL Compiled: Sep  2 2011 18:34:46 (0001ms, 0572ms total)
T0C10 000:573 Logging started @ 2011-10-12 12:56 (0001ms, 0572ms total)
T0C10 000:574 JLINK_SetWarnOutHandler(...) (0000ms, 0573ms total)
T0C10 000:574 JLINK_OpenEx(...)
Firmware: J-Link ARM V8 compiled Sep  2 2011 17:54:36
Hardware: V8.00
S/N: 20100214
Feature(s): RDI,FlashDL,FlashBP,JFlash,GDBFull  returns O.K. (0323ms, 0573ms total)
T0C10 000:897 JLINK_SetErrorOutHandler(...) (0000ms, 0896ms total)
T0C10 000:897 JLINK_ExecCommand("Device = LM3S9B92", ...)
                JLINK_ExecCommand("map ram 0x20000000 - 0x20017FFF", ...)  returns 0x00 (0000ms, 0000ms total)
                JLINK_AddMirrorAreaEx(Addr = 0x00000000, Size = 0x00000000) (0001ms, 0000ms total)
              Device "LM3S9B92" selected (256 KB flash, 96 KB RAM).  returns 0x00 (0005ms, 0896ms total)
T0C10 000:904 JLINK_ExecCommand("ProjectFile = "E:\Mywork\ARM\LM3S9B92\LM3S9B92-Simple-CD\Code\StellarisWare\boards\Smart-9B92-C3\timers\JLinkSettings.ini"", ...)  returns 0x00 (0001ms, 0901ms total)
T0C10 000:907 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x00 (0000ms, 0902ms total)
T0C10 000:907 JLINK_TIF_Select(JLINKARM_TIF_JTAG)  returns 0x00 (0000ms, 0902ms total)
T0C10 000:907 JLINK_SetSpeed(2000) (0001ms, 0902ms total)
T0C10 000:908 JLINK_GetHardwareVersion()  returns 0x13880 (0000ms, 0903ms total)
T0C10 000:908 JLINK_GetDLLVersion()  returns 43502 (0000ms, 0903ms total)
T0C10 000:908 JLINK_GetFirmwareString(...) (0000ms, 0903ms total)
T0C10 000:915 JLINK_GetDLLVersion()  returns 43502 (0000ms, 0903ms total)
T0C10 000:915 JLINK_GetCompileDateTime() (0000ms, 0903ms total)
T0C10 000:918 JLINK_GetFirmwareString(...) (0000ms, 0903ms total)
T0C10 000:920 JLINK_GetHardwareVersion()  returns 0x13880 (0000ms, 0903ms total)
T0C10 000:928 JLINK_GetIdData(...) >0x2F8 JTAG>TotalIRLen = 4, IRPrint = 0x01 >0x30 JTAG> >0x210 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x30 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>Found Cortex-M3 r2p0, Little endian. >0x48 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>TPIU fitted. >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>  FPUnit: 6 code (BP) slots and 2 literal slots >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> ScanLen=4
 NumDevices=1 aId[0]=0x4BA00477 aIrRead[0]=0 aScanLen[0]=0 aScanRead[0]=0 (0080ms, 0903ms total)
T0C10 001:009 JLINK_JTAG_GetDeviceID(DeviceIndex = 0)  returns 0x4BA00477 (0000ms, 0983ms total)
T0C10 001:009 JLINK_JTAG_GetDeviceInfo(DeviceIndex = 0)  returns 0x00 (0000ms, 0983ms total)
T0C10 001:009 JLINK_GetDebugInfo(0x100) -- Value=0xE00FF003  returns 0x00 (0001ms, 0983ms total)
T0C10 001:012 JLINK_ReadMem (0xE00FFFF0, 0x0010 Bytes, ...) -- CPU is running -- CPU_ReadMem(16 bytes @ 0xE00FFFF0) -- Data:  0D 00 00 00 10 00 00 00 05 00 00 00 B1 00 00 00  returns 0x00 (0005ms, 0984ms total)
T0C10 001:017 JLINK_ReadMem (0xE00FFFD0, 0x0020 Bytes, ...) -- CPU is running -- CPU_ReadMem(32 bytes @ 0xE00FFFD0) -- Data:  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x00 (0001ms, 0989ms total)
T0C10 001:018 JLINK_ReadMem (0xE00FF000, 0x0018 Bytes, ...) -- CPU is running -- CPU_ReadMem(24 bytes @ 0xE00FF000) -- Data:  03 F0 F0 FF 03 20 F0 FF 03 30 F0 FF 03 10 F0 FF ...  returns 0x00 (0002ms, 0990ms total)
T0C10 001:020 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000ED00) -- Data:  30 C2 2F 41  returns 0x01 (0001ms, 0992ms total)
T0C10 001:021 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 0993ms total)
T0C10 001:021 JLINK_Reset() >0x300 JTAG>TotalIRLen = 4, IRPrint = 0x01 >0x30 JTAG> >0x210 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x30 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>Found Cortex-M3 r2p0, Little endian. >0x48 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>TPIU fitted. >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>  FPUnit: 6 code (BP) slots and 2 literal slots >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) >0x80 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_WriteMem(4 bytes @ 0xE0001028) -- CPU_WriteMem(4 bytes @ 0xE0001038) -- CPU_WriteMem(4 bytes @ 0xE0001048) -- CPU_WriteMem(4 bytes @ 0xE0001058) (0107ms, 0993ms total)
T0C10 001:128 JLINK_Halt()  returns 0x00 (0000ms, 1100ms total)
T0C10 001:128 JLINK_IsHalted()  returns TRUE (0000ms, 1100ms total)
T0C10 001:128 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- Data:  03 00 03 00  returns 0x01 (0001ms, 1100ms total)
T0C10 001:129 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0x00 (0001ms, 1101ms total)
T0C10 001:130 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0001ms, 1102ms total)
T0C10 001:131 JLINK_ReadMemU32(0xE0002000, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0002000) -- Data:  60 02 00 00  returns 0x01 (0001ms, 1103ms total)
T0C10 001:132 JLINK_ReadMemU32(0xE0001000, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- Data:  00 00 00 40  returns 0x01 (0001ms, 1104ms total)
T0C10 001:133 JLINK_WriteU32(0xE0001028, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001028)  returns 0x00 (0001ms, 1105ms total)
T0C10 001:134 JLINK_WriteU32(0xE0001038, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001038)  returns 0x00 (0001ms, 1106ms total)
T0C10 001:135 JLINK_WriteU32(0xE0001048, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001048)  returns 0x00 (0000ms, 1107ms total)
T0C10 001:135 JLINK_WriteU32(0xE0001058, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001058)  returns 0x00 (0001ms, 1107ms total)
T0C10 001:146 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 1108ms total)
T0C10 001:157 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x06 (0000ms, 1109ms total)
T0C10 001:157 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 1109ms total)
T0C10 001:157 JLINK_GetNumWPUnits()  returns 0x04 (0000ms, 1109ms total)
T0C10 001:164 JLINK_GetSpeed()  returns 0x7D0 (0000ms, 1109ms total)
T0C10 001:169 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) -- Data:  01 00 00 00  returns 0x01 (0001ms, 1109ms total)
T0C10 001:170 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) -- Data:  01 00 00 00  returns 0x01 (0001ms, 1110ms total)
T0C10 001:171 JLINK_WriteMem(0xE0001000, 0x001C Bytes, ...) -- Data:  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ... -- CPU_WriteMem(28 bytes @ 0xE0001000)  returns 0x1C (0001ms, 1111ms total)
T0C10 001:172 JLINK_ReadMem (0xE0001000, 0x001C Bytes, ...) -- CPU_ReadMem(28 bytes @ 0xE0001000) -- Data:  01 00 00 40 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x00 (0002ms, 1112ms total)
T0C10 001:174 JLINK_Halt()  returns 0x00 (0000ms, 1114ms total)
T0C10 001:174 JLINK_IsHalted()  returns TRUE (0000ms, 1114ms total)
T0C10 001:178 JLINK_WriteMem(0x20000000, 0x0134 Bytes, ...) -- Data:  00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(308 bytes @ 0x20000000)  returns 0x134 (0003ms, 1114ms total)
T0C10 001:181 JLINK_WriteReg(R0, 0x00000000)  returns 0x00 (0000ms, 1117ms total)
T0C10 001:181 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 1117ms total)
T0C10 001:181 JLINK_WriteReg(R2, 0x00000001)  returns 0x00 (0000ms, 1117ms total)
T0C10 001:181 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1117ms total)
T0C10 001:181 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1117ms total)
T0C10 001:181 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1117ms total)
T0C10 001:181 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0001ms, 1117ms total)
T0C10 001:182 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(R15, 0x20000038)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1118ms total)
T0C10 001:182 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000001 (0002ms, 1118ms total)
T0C10 001:184 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 1120ms total)
T0C10 001:192 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0007ms, 1128ms total)
T0C10 001:199 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1128ms total)
T0C10 001:199 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:199 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R0, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(R15, 0x20000020)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1128ms total)
T0C10 001:200 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0001ms, 1128ms total)
T0C10 001:201 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1129ms total)
T0C10 001:201 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1129ms total)
T0C10 001:201 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1129ms total)
T0C10 001:201 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1129ms total)
T0C10 001:201 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1129ms total)
T0C10 001:201 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000002 (0000ms, 1129ms total)
T0C10 001:201 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0006ms, 1129ms total)
T0C10 001:207 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1135ms total)
T0C10 001:213 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1135ms total)
T0C10 001:213 JLINK_ClrBPEx(BPHandle = 0x00000002)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_ReadReg(R0)  returns 0x00000001 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R0, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(R15, 0x20000088)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1135ms total)
T0C10 001:214 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0001ms, 1135ms total)
T0C10 001:215 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1136ms total)
T0C10 001:215 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1136ms total)
T0C10 001:215 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000003 (0000ms, 1136ms total)
T0C10 001:215 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 1136ms total)
T0C10 001:222 JLINK_IsHalted()  returns FALSE (0001ms, 1143ms total)
T0C10 001:273 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1143ms total)
T0C10 001:279 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1143ms total)
T0C10 001:279 JLINK_ClrBPEx(BPHandle = 0x00000003)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:279 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R0, 0x00000400)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(R15, 0x20000020)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1143ms total)
T0C10 001:280 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0001ms, 1143ms total)
T0C10 001:281 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1144ms total)
T0C10 001:281 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1144ms total)
T0C10 001:281 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1144ms total)
T0C10 001:281 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1144ms total)
T0C10 001:281 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000004 (0000ms, 1144ms total)
T0C10 001:281 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 1144ms total)
T0C10 001:288 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0007ms, 1151ms total)
T0C10 001:295 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1151ms total)
T0C10 001:295 JLINK_ClrBPEx(BPHandle = 0x00000004)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_ReadReg(R0)  returns 0x00000001 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R0, 0x00000400)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(R15, 0x20000088)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1151ms total)
T0C10 001:295 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0001ms, 1151ms total)
T0C10 001:296 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1152ms total)
T0C10 001:296 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1152ms total)
T0C10 001:296 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1152ms total)
T0C10 001:296 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1152ms total)
T0C10 001:296 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1152ms total)
T0C10 001:296 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000005 (0000ms, 1152ms total)
T0C10 001:296 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 1152ms total)
T0C10 001:303 JLINK_IsHalted()  returns FALSE (0001ms, 1159ms total)
T0C10 001:354 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1159ms total)
T0C10 001:360 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1159ms total)
T0C10 001:360 JLINK_ClrBPEx(BPHandle = 0x00000005)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:360 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R0, 0x00000001)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(R15, 0x20000058)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1159ms total)
T0C10 001:361 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000006 (0000ms, 1159ms total)
T0C10 001:361 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 1159ms total)
T0C10 001:369 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1167ms total)
T0C10 001:375 JLINK_ReadReg(R15)  returns 0x20000000 (0001ms, 1167ms total)
T0C10 001:376 JLINK_ClrBPEx(BPHandle = 0x00000006)  returns 0x00 (0000ms, 1168ms total)
T0C10 001:376 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1168ms total)
T0C10 001:436 JLINK_WriteMem(0x20000000, 0x0134 Bytes, ...) -- Data:  00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(308 bytes @ 0x20000000)  returns 0x134 (0003ms, 1168ms total)
T0C10 001:439 JLINK_WriteReg(R0, 0x00000000)  returns 0x00 (0001ms, 1171ms total)
T0C10 001:440 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R2, 0x00000002)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(R15, 0x20000038)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1172ms total)
T0C10 001:440 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000007 (0001ms, 1172ms total)
T0C10 001:441 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 1173ms total)
T0C10 001:449 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1181ms total)
T0C10 001:455 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1181ms total)
T0C10 001:455 JLINK_ClrBPEx(BPHandle = 0x00000007)  returns 0x00 (0001ms, 1181ms total)
T0C10 001:456 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1182ms total)
T0C10 001:456 JLINK_WriteMem(0x20000134, 0x0400 Bytes, ...) -- Data:  10 01 00 20 1D 01 00 00 21 01 00 00 23 01 00 00 ... -- CPU_WriteMem(1024 bytes @ 0x20000134)  returns 0x400 (0007ms, 1182ms total)
T0C10 001:463 JLINK_WriteReg(R0, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R2, 0x20000134)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(R15, 0x200000AA)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:463 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1189ms total)
T0C10 001:464 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1190ms total)
T0C10 001:464 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1190ms total)
T0C10 001:464 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1190ms total)
T0C10 001:464 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1190ms total)
T0C10 001:464 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1190ms total)
T0C10 001:464 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1190ms total)
T0C10 001:464 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000008 (0000ms, 1190ms total)
T0C10 001:464 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 1190ms total)
T0C10 001:471 JLINK_IsHalted()  returns FALSE (0001ms, 1197ms total)
T0C10 001:522 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1197ms total)
T0C10 001:528 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1197ms total)
T0C10 001:528 JLINK_ClrBPEx(BPHandle = 0x00000008)  returns 0x00 (0000ms, 1197ms total)
T0C10 001:528 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1197ms total)
T0C10 001:529 JLINK_WriteMem(0x20000134, 0x0400 Bytes, ...) -- Data:  48 D3 F8 E7 01 CD 00 21 0A 22 00 90 03 E0 01 CD ... -- CPU_WriteMem(1024 bytes @ 0x20000134)  returns 0x400 (0007ms, 1197ms total)
T0C10 001:536 JLINK_WriteReg(R0, 0x00000400)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R1, 0x000002C0)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R2, 0x20000134)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1204ms total)
T0C10 001:536 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0001ms, 1204ms total)
T0C10 001:537 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(R15, 0x200000AA)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1205ms total)
T0C10 001:537 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000009 (0000ms, 1205ms total)
T0C10 001:537 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 1205ms total)
T0C10 001:545 JLINK_IsHalted()  returns FALSE (0000ms, 1213ms total)
T0C10 001:595 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1213ms total)
T0C10 001:601 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1213ms total)
T0C10 001:601 JLINK_ClrBPEx(BPHandle = 0x00000009)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R0, 0x00000002)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R1, 0x000002C0)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R2, 0x20000134)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:601 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(R15, 0x20000058)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1213ms total)
T0C10 001:602 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000A (0000ms, 1213ms total)
T0C10 001:602 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 1213ms total)
T0C10 001:610 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1221ms total)
T0C10 001:616 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1221ms total)
T0C10 001:616 JLINK_ClrBPEx(BPHandle = 0x0000000A)  returns 0x00 (0000ms, 1221ms total)
T0C10 001:616 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1221ms total)
T0C10 001:674 JLINK_WriteMem(0x20000000, 0x0134 Bytes, ...) -- Data:  00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(308 bytes @ 0x20000000)  returns 0x134 (0003ms, 1221ms total)
T0C10 001:677 JLINK_WriteReg(R0, 0x00000000)  returns 0x00 (0001ms, 1224ms total)
T0C10 001:678 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R2, 0x00000003)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(R15, 0x20000038)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1225ms total)
T0C10 001:678 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x0000000B (0001ms, 1225ms total)
T0C10 001:679 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 1226ms total)
T0C10 001:687 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1234ms total)
T0C10 001:693 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1234ms total)
T0C10 001:693 JLINK_ClrBPEx(BPHandle = 0x0000000B)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R0, 0xFFFFFFFF)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R1, 0x00000000)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R2, 0x000006C0)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R3, 0x04C11DB7)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1234ms total)
T0C10 001:693 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0001ms, 1234ms total)
T0C10 001:694 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(R15, 0x20000002)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1235ms total)
T0C10 001:694 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000C (0000ms, 1235ms total)
T0C10 001:694 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0009ms, 1235ms total)
T0C10 001:703 JLINK_IsHalted()  returns FALSE (0001ms, 1244ms total)
T0C10 001:754 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 1244ms total)
T0C10 001:760 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1244ms total)
T0C10 001:760 JLINK_ClrBPEx(BPHandle = 0x0000000C)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:760 JLINK_ReadReg(R0)  returns 0x061BB9A1 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R0, 0x00000003)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R1, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R2, 0x000006C0)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R3, 0x04C11DB7)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(R15, 0x20000058)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:762 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 1244ms total)
T0C10 001:763 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 1245ms total)
T0C10 001:763 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 1245ms total)
T0C10 001:763 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 1245ms total)
T0C10 001:763 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000D (0000ms, 1245ms total)
T0C10 001:763 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0006ms, 1245ms total)
T0C10 001:769 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0007ms, 1251ms total)
T0C10 001:776 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 1251ms total)
T0C10 001:776 JLINK_ClrBPEx(BPHandle = 0x0000000D)  returns 0x00 (0000ms, 1251ms total)
T0C10 001:776 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 1251ms total)
T0C10 001:830 JLINK_WriteU32(0xE000EDFC, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0001ms, 1251ms total)
T0C10 001:831 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 1252ms total)
T0C10 001:831 JLINK_Reset() >0x2F8 JTAG>TotalIRLen = 4, IRPrint = 0x01 >0x30 JTAG> >0x210 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x30 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>Found Cortex-M3 r2p0, Little endian. >0x48 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>TPIU fitted. >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>  FPUnit: 6 code (BP) slots and 2 literal slots >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) >0x80 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE0001028) -- CPU_WriteMem(4 bytes @ 0xE0001038) -- CPU_WriteMem(4 bytes @ 0xE0001048) -- CPU_WriteMem(4 bytes @ 0xE0001058)
 (0108ms, 1252ms total)
