
T1CE4 007:923 SEGGER J-Link V4.35b (beta) Log File (0012ms, 7923ms total)
T1CE4 007:923 DLL Compiled: Sep  2 2011 18:34:46 (0012ms, 7923ms total)
T1CE4 007:923 Logging started @ 2011-10-11 12:03 (0013ms, 7923ms total)
T1CE4 007:936 JLINK_SetWarnOutHandler(...) (0000ms, 7936ms total)
T1CE4 007:936 JLINK_OpenEx(...)
Firmware: J-Link ARM V8 compiled Sep  2 2011 17:54:36
Hardware: V8.00
S/N: 20100214
Feature(s): RDI,FlashDL,FlashBP,JFlash,GDBFull  returns O.K. (0464ms, 7936ms total)
T1CE4 008:400 JLINK_SetErrorOutHandler(...) (0000ms, 8400ms total)
T1CE4 008:400 JLINK_ExecCommand("Device = LM3S9B92", ...)
                JLINK_ExecCommand("map ram 0x20000000 - 0x20017FFF", ...)  returns 0x00 (0000ms, 0000ms total)
                JLINK_AddMirrorAreaEx(Addr = 0x00000000, Size = 0x00000000) (0000ms, 0000ms total)
              Device "LM3S9B92" selected (256 KB flash, 96 KB RAM).  returns 0x00 (0005ms, 8400ms total)
T1CE4 008:407 JLINK_ExecCommand("ProjectFile = "E:\Mywork\ARM\LM3S9B92\LM3S9B92-Simple-CD\Code\StellarisWare\boards\Smart-9B92-C1\blinky\JLinkSettings.ini"", ...)  returns 0x00 (0006ms, 8405ms total)
T1CE4 008:427 JLINK_ExecCommand("DisableConnectionTimeout", ...)  returns 0x00 (0000ms, 8411ms total)
T1CE4 008:427 JLINK_TIF_Select(JLINKARM_TIF_JTAG)  returns 0x00 (0000ms, 8411ms total)
T1CE4 008:427 JLINK_SetSpeed(2000) (0000ms, 8411ms total)
T1CE4 008:427 JLINK_GetHardwareVersion()  returns 0x13880 (0000ms, 8411ms total)
T1CE4 008:427 JLINK_GetDLLVersion()  returns 43502 (0000ms, 8411ms total)
T1CE4 008:427 JLINK_GetFirmwareString(...) (0000ms, 8411ms total)
T1CE4 008:505 JLINK_GetDLLVersion()  returns 43502 (0000ms, 8411ms total)
T1CE4 008:505 JLINK_GetCompileDateTime() (0000ms, 8411ms total)
T1CE4 008:524 JLINK_GetFirmwareString(...) (0001ms, 8411ms total)
T1CE4 008:541 JLINK_GetHardwareVersion()  returns 0x13880 (0000ms, 8412ms total)
T1CE4 008:599 JLINK_GetIdData(...) >0x2F8 JTAG>TotalIRLen = 4, IRPrint = 0x01 >0x30 JTAG> >0x210 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x30 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>Found Cortex-M3 r2p0, Little endian. >0x48 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>TPIU fitted. >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>  FPUnit: 6 code (BP) slots and 2 literal slots >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> ScanLen=4
 NumDevices=1 aId[0]=0x4BA00477 aIrRead[0]=0 aScanLen[0]=0 aScanRead[0]=0 (0107ms, 8412ms total)
T1CE4 008:706 JLINK_JTAG_GetDeviceID(DeviceIndex = 0)  returns 0x4BA00477 (0000ms, 8519ms total)
T1CE4 008:706 JLINK_JTAG_GetDeviceInfo(DeviceIndex = 0)  returns 0x00 (0000ms, 8519ms total)
T1CE4 008:706 JLINK_GetDebugInfo(0x100) -- Value=0xE00FF003  returns 0x00 (0000ms, 8519ms total)
T1CE4 008:709 JLINK_ReadMem (0xE00FFFF0, 0x0010 Bytes, ...) -- CPU is running -- CPU_ReadMem(16 bytes @ 0xE00FFFF0) -- Data:  0D 00 00 00 10 00 00 00 05 00 00 00 B1 00 00 00  returns 0x00 (0004ms, 8519ms total)
T1CE4 008:713 JLINK_ReadMem (0xE00FFFD0, 0x0020 Bytes, ...) -- CPU is running -- CPU_ReadMem(32 bytes @ 0xE00FFFD0) -- Data:  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x00 (0001ms, 8523ms total)
T1CE4 008:714 JLINK_ReadMem (0xE00FF000, 0x0018 Bytes, ...) -- CPU is running -- CPU_ReadMem(24 bytes @ 0xE00FF000) -- Data:  03 F0 F0 FF 03 20 F0 FF 03 30 F0 FF 03 10 F0 FF ...  returns 0x00 (0001ms, 8524ms total)
T1CE4 008:715 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000ED00) -- Data:  30 C2 2F 41  returns 0x01 (0001ms, 8525ms total)
T1CE4 008:716 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 8526ms total)
T1CE4 008:716 JLINK_Reset() >0x300 JTAG>TotalIRLen = 4, IRPrint = 0x01 >0x30 JTAG> >0x210 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x30 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>Found Cortex-M3 r2p0, Little endian. >0x48 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>TPIU fitted. >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>  FPUnit: 6 code (BP) slots and 2 literal slots >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running
 -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) >0x80 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_WriteMem(4 bytes @ 0xE0001028) -- CPU_WriteMem(4 bytes @ 0xE0001038) -- CPU_WriteMem(4 bytes @ 0xE0001048) -- CPU_WriteMem(4 bytes @ 0xE0001058) (0111ms, 8526ms total)
T1CE4 008:827 JLINK_WriteU32(0xE000EDFC, 0x00000001) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0000ms, 8637ms total)
T1CE4 008:827 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- Data:  03 00 03 00  returns 0x01 (0001ms, 8637ms total)
T1CE4 008:829 JLINK_ReadMemU32(0x400FE060, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0x400FE060) -- Data:  D1 3A AE 07  returns 0x01 (0001ms, 8638ms total)
T1CE4 008:830 JLINK_WriteU32(0x400FE060, 0x07AE3AD1) -- CPU_WriteMem(4 bytes @ 0x400FE060)  returns 0x00 (0000ms, 8639ms total)
T1CE4 008:830 JLINK_WriteU32(0xE000ED0C, 0x05FA0001) -- CPU_WriteMem(4 bytes @ 0xE000ED0C)  returns 0x00 (0001ms, 8639ms total)
T1CE4 008:831 JLINK_Halt()  returns 0x00 (0001ms, 8640ms total)
T1CE4 008:832 JLINK_IsHalted()  returns TRUE (0000ms, 8641ms total)
T1CE4 008:832 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- Data:  03 00 03 02  returns 0x01 (0001ms, 8641ms total)
T1CE4 008:833 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0x00 (0000ms, 8642ms total)
T1CE4 008:834 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0000ms, 8642ms total)
T1CE4 008:834 JLINK_ReadMemU32(0xE0002000, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0002000) -- Data:  60 02 00 00  returns 0x01 (0002ms, 8642ms total)
T1CE4 008:836 JLINK_ReadMemU32(0xE0001000, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- Data:  00 00 00 40  returns 0x01 (0001ms, 8644ms total)
T1CE4 008:837 JLINK_WriteU32(0xE0001028, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001028)  returns 0x00 (0000ms, 8645ms total)
T1CE4 008:837 JLINK_WriteU32(0xE0001038, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001038)  returns 0x00 (0001ms, 8645ms total)
T1CE4 008:838 JLINK_WriteU32(0xE0001048, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001048)  returns 0x00 (0001ms, 8646ms total)
T1CE4 008:839 JLINK_WriteU32(0xE0001058, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE0001058)  returns 0x00 (0001ms, 8647ms total)
T1CE4 008:849 JLINK_GetHWStatus(...)  returns 0x00 (0001ms, 8648ms total)
T1CE4 008:859 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x06 (0000ms, 8649ms total)
T1CE4 008:859 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 8649ms total)
T1CE4 008:859 JLINK_GetNumWPUnits()  returns 0x04 (0000ms, 8649ms total)
T1CE4 008:865 JLINK_GetSpeed()  returns 0x7D0 (0000ms, 8649ms total)
T1CE4 008:872 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) -- Data:  01 00 00 00  returns 0x01 (0001ms, 8649ms total)
T1CE4 008:874 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) -- Data:  01 00 00 00  returns 0x01 (0001ms, 8651ms total)
T1CE4 008:875 JLINK_WriteMem(0xE0001000, 0x001C Bytes, ...) -- Data:  01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ... -- CPU_WriteMem(28 bytes @ 0xE0001000)  returns 0x1C (0001ms, 8652ms total)
T1CE4 008:876 JLINK_ReadMem (0xE0001000, 0x001C Bytes, ...) -- CPU_ReadMem(28 bytes @ 0xE0001000) -- Data:  01 00 00 40 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x00 (0001ms, 8653ms total)
T1CE4 008:877 JLINK_ReadMemU32(0x400FE000, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0x400FE000) -- Data:  01 02 04 10  returns 0x01 (0001ms, 8654ms total)
T1CE4 008:878 JLINK_Halt()  returns 0x00 (0000ms, 8655ms total)
T1CE4 008:878 JLINK_IsHalted()  returns TRUE (0000ms, 8655ms total)
T1CE4 008:880 JLINK_WriteMem(0x20000000, 0x0134 Bytes, ...) -- Data:  00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(308 bytes @ 0x20000000)  returns 0x134 (0004ms, 8655ms total)
T1CE4 008:884 JLINK_WriteReg(R0, 0x00001000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R2, 0x00000001)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8659ms total)
T1CE4 008:884 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0001ms, 8659ms total)
T1CE4 008:885 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8660ms total)
T1CE4 008:885 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8660ms total)
T1CE4 008:885 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8660ms total)
T1CE4 008:885 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8660ms total)
T1CE4 008:885 JLINK_WriteReg(R15, 0x20000038)  returns 0x00 (0000ms, 8660ms total)
T1CE4 008:885 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8660ms total)
T1CE4 008:885 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0001ms, 8660ms total)
T1CE4 008:886 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8661ms total)
T1CE4 008:886 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8661ms total)
T1CE4 008:886 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8661ms total)
T1CE4 008:886 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8661ms total)
T1CE4 008:886 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8661ms total)
T1CE4 008:886 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000001 (0001ms, 8661ms total)
T1CE4 008:887 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0009ms, 8662ms total)
T1CE4 008:896 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8671ms total)
T1CE4 008:902 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8671ms total)
T1CE4 008:902 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 8671ms total)
T1CE4 008:902 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8671ms total)
T1CE4 008:902 JLINK_WriteReg(R0, 0x00001000)  returns 0x00 (0001ms, 8671ms total)
T1CE4 008:903 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:903 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(R15, 0x20000020)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000002 (0000ms, 8672ms total)
T1CE4 008:904 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 8672ms total)
T1CE4 008:912 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8680ms total)
T1CE4 008:918 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_ClrBPEx(BPHandle = 0x00000002)  returns 0x00 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_ReadReg(R0)  returns 0x00000001 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_WriteReg(R0, 0x00001000)  returns 0x00 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8680ms total)
T1CE4 008:918 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0001ms, 8680ms total)
T1CE4 008:919 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:919 JLINK_WriteReg(R15, 0x20000088)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000003 (0000ms, 8681ms total)
T1CE4 008:920 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 8681ms total)
T1CE4 008:927 JLINK_IsHalted()  returns FALSE (0001ms, 8688ms total)
T1CE4 008:978 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8688ms total)
T1CE4 008:984 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8688ms total)
T1CE4 008:984 JLINK_ClrBPEx(BPHandle = 0x00000003)  returns 0x00 (0000ms, 8688ms total)
T1CE4 008:984 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8688ms total)
T1CE4 008:984 JLINK_WriteReg(R0, 0x00000001)  returns 0x00 (0000ms, 8688ms total)
T1CE4 008:984 JLINK_WriteReg(R1, 0x00000400)  returns 0x00 (0001ms, 8688ms total)
T1CE4 008:985 JLINK_WriteReg(R2, 0x000000FF)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(R15, 0x20000058)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8689ms total)
T1CE4 008:985 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0001ms, 8689ms total)
T1CE4 008:986 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8690ms total)
T1CE4 008:986 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8690ms total)
T1CE4 008:986 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8690ms total)
T1CE4 008:986 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000004 (0000ms, 8690ms total)
T1CE4 008:986 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 8690ms total)
T1CE4 008:993 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8697ms total)
T1CE4 008:999 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8697ms total)
T1CE4 008:999 JLINK_ClrBPEx(BPHandle = 0x00000004)  returns 0x00 (0000ms, 8697ms total)
T1CE4 008:999 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8697ms total)
T1CE4 009:054 JLINK_WriteMem(0x20000000, 0x0134 Bytes, ...) -- Data:  00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(308 bytes @ 0x20000000)  returns 0x134 (0003ms, 8697ms total)
T1CE4 009:057 JLINK_WriteReg(R0, 0x00001000)  returns 0x00 (0000ms, 8700ms total)
T1CE4 009:057 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0001ms, 8700ms total)
T1CE4 009:058 JLINK_WriteReg(R2, 0x00000002)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(R15, 0x20000038)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8701ms total)
T1CE4 009:058 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0001ms, 8701ms total)
T1CE4 009:059 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000005 (0001ms, 8702ms total)
T1CE4 009:060 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 8703ms total)
T1CE4 009:068 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8711ms total)
T1CE4 009:074 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8711ms total)
T1CE4 009:074 JLINK_ClrBPEx(BPHandle = 0x00000005)  returns 0x00 (0000ms, 8711ms total)
T1CE4 009:074 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8711ms total)
T1CE4 009:075 JLINK_WriteMem(0x20000134, 0x0400 Bytes, ...) -- Data:  00 01 00 20 1D 11 00 00 21 11 00 00 23 11 00 00 ... -- CPU_WriteMem(1024 bytes @ 0x20000134)  returns 0x400 (0007ms, 8711ms total)
T1CE4 009:082 JLINK_WriteReg(R0, 0x00001000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R1, 0x000001E8)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R2, 0x20000134)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(R15, 0x200000AA)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000006 (0000ms, 8718ms total)
T1CE4 009:082 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 8718ms total)
T1CE4 009:090 JLINK_IsHalted()  returns FALSE (0001ms, 8726ms total)
T1CE4 009:141 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8726ms total)
T1CE4 009:147 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_ClrBPEx(BPHandle = 0x00000006)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_WriteReg(R0, 0x00000002)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_WriteReg(R1, 0x000001E8)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_WriteReg(R2, 0x20000134)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:147 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8726ms total)
T1CE4 009:148 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(R15, 0x20000058)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000007 (0000ms, 8727ms total)
T1CE4 009:148 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 8727ms total)
T1CE4 009:156 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8735ms total)
T1CE4 009:163 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8735ms total)
T1CE4 009:163 JLINK_ClrBPEx(BPHandle = 0x00000007)  returns 0x00 (0000ms, 8735ms total)
T1CE4 009:163 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8735ms total)
T1CE4 009:219 JLINK_WriteMem(0x20000000, 0x0134 Bytes, ...) -- Data:  00 BE 0A E0 0D 78 2D 06 68 40 08 24 40 00 00 D3 ... -- CPU_WriteMem(308 bytes @ 0x20000000)  returns 0x134 (0003ms, 8735ms total)
T1CE4 009:223 JLINK_WriteReg(R0, 0x00001000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R1, 0x007A1200)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R2, 0x00000003)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R3, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(R15, 0x20000038)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8738ms total)
T1CE4 009:223 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2) -- CPU_ReadMem(2 bytes @ 0x20000000)  returns 0x00000008 (0002ms, 8738ms total)
T1CE4 009:225 JLINK_Go() -- CPU_WriteMem(2 bytes @ 0x20000000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0007ms, 8740ms total)
T1CE4 009:232 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0007ms, 8747ms total)
T1CE4 009:239 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_ClrBPEx(BPHandle = 0x00000008)  returns 0x00 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_WriteReg(R0, 0xFFFFFFFF)  returns 0x00 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_WriteReg(R1, 0x00001000)  returns 0x00 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_WriteReg(R2, 0x000001E8)  returns 0x00 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_WriteReg(R3, 0x04C11DB7)  returns 0x00 (0000ms, 8747ms total)
T1CE4 009:239 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0001ms, 8747ms total)
T1CE4 009:240 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(R15, 0x20000002)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x00000009 (0000ms, 8748ms total)
T1CE4 009:240 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 8748ms total)
T1CE4 009:248 JLINK_IsHalted()  returns FALSE (0000ms, 8756ms total)
T1CE4 009:298 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8756ms total)
T1CE4 009:304 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8756ms total)
T1CE4 009:304 JLINK_ClrBPEx(BPHandle = 0x00000009)  returns 0x00 (0000ms, 8756ms total)
T1CE4 009:304 JLINK_ReadReg(R0)  returns 0x129E541E (0000ms, 8756ms total)
T1CE4 009:304 JLINK_WriteReg(R0, 0x00000003)  returns 0x00 (0000ms, 8756ms total)
T1CE4 009:304 JLINK_WriteReg(R1, 0x00001000)  returns 0x00 (0000ms, 8756ms total)
T1CE4 009:304 JLINK_WriteReg(R2, 0x000001E8)  returns 0x00 (0000ms, 8756ms total)
T1CE4 009:304 JLINK_WriteReg(R3, 0x04C11DB7)  returns 0x00 (0000ms, 8756ms total)
T1CE4 009:304 JLINK_WriteReg(R4, 0x00000000)  returns 0x00 (0001ms, 8756ms total)
T1CE4 009:305 JLINK_WriteReg(R5, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R6, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R7, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R8, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R9, 0x20000130)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R10, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R11, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R12, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R13, 0x20000800)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R14, 0x20000001)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(R15, 0x20000058)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(XPSR, 0x01000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(MSP, 0x20000800)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(PSP, 0x20000800)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(BASEPRI, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(CONTROL, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(FAULTMASK, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_WriteReg(BASEPRI_MAX, 0x00000000)  returns 0x00 (0000ms, 8757ms total)
T1CE4 009:305 JLINK_SetBPEx(Addr = 0x20000000, Type = 0xFFFFFFF2)  returns 0x0000000A (0000ms, 8757ms total)
T1CE4 009:305 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) (0008ms, 8757ms total)
T1CE4 009:313 JLINK_IsHalted() -- CPU_ReadMem(2 bytes @ 0x20000000)  returns TRUE (0006ms, 8765ms total)
T1CE4 009:319 JLINK_ReadReg(R15)  returns 0x20000000 (0000ms, 8765ms total)
T1CE4 009:319 JLINK_ClrBPEx(BPHandle = 0x0000000A)  returns 0x00 (0000ms, 8765ms total)
T1CE4 009:319 JLINK_ReadReg(R0)  returns 0x00000000 (0000ms, 8765ms total)
T1CE4 009:371 JLINK_WriteU32(0xE000EDFC, 0x00000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0001ms, 8765ms total)
T1CE4 009:372 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 8766ms total)
T1CE4 009:372 JLINK_Reset() >0x2F8 JTAG>TotalIRLen = 4, IRPrint = 0x01 >0x30 JTAG> >0x210 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x30 JTAG> >0x78 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>Found Cortex-M3 r2p0, Little endian. >0x48 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x30 JTAG> >0x48 JTAG> >0x40 JTAG> >0x78 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG>
 >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>TPIU fitted. >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG>  FPUnit: 6 code (BP) slots and 2 literal slots >0x40 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_WriteMem(4 bytes @ 0xE000ED0C) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU is running -- CPU_ReadMem(4 bytes @ 0xE000EDF0) >0x80 JTAG> >0x40 JTAG> >0x30 JTAG> >0x40 JTAG> >0x48 JTAG> >0x40 JTAG> -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE0001028) -- CPU_WriteMem(4 bytes @ 0xE0001038) -- CPU_WriteMem(4 bytes @ 0xE0001048) -- CPU_WriteMem(4 bytes @ 0xE0001058)
 (0122ms, 8766ms total)
T1CE4 009:494 JLINK_WriteU32(0xE000EDFC, 0x00000001) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0x00 (0001ms, 8888ms total)
T1CE4 009:495 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- Data:  03 00 03 00  returns 0x01 (0001ms, 8889ms total)
T1CE4 009:496 JLINK_ReadMemU32(0x400FE060, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0x400FE060) -- Data:  D1 3A AE 07  returns 0x01 (0001ms, 8890ms total)
T1CE4 009:497 JLINK_WriteU32(0x400FE060, 0x07AE3AD1) -- CPU_WriteMem(4 bytes @ 0x400FE060)  returns 0x00 (0001ms, 8891ms total)
T1CE4 009:498 JLINK_WriteU32(0xE000ED0C, 0x05FA0004) -- CPU_WriteMem(4 bytes @ 0xE000ED0C)  returns 0x00 (0001ms, 8892ms total)
