This is a HTTP Server example. It shows you how to use the
Web Server CGI interface as well. 

Use this example to connect LM3S9B92 Board to a LAN with DHCP
server (most LANs have this). This example will configure the 
LAN network parameters automatically using a DHCP protocol.

You may connect Luminary Board to PC directly over a crosslink
network cable. In this case configure a PC to use a static 
IP address 192.168.0.1

If after a timeout of 5 seconds DHCP did not obtain an IP address,
this example will use a static IP address 192.168.0.100

The WEB pages are included into the project under HTTP Files 
group. You can simply add or remove a page or image. Web files
which are compiled into the project are added to the 'Web.inp'
Web Converter input file.

To test this example, open your web browser and enter the 
address http://stellaris/ or http://<boards IP address>

Default user    : admin
Default password: <none>

You can change the password at runtime on page 'system'

The HTTP_demo example is available for several targets:

LM3S9B92:       Standalone (no RTX Kernel) application.
                Program code is loaded into on-chip flash.

LM3S9B92 Debug: Standalone (no RTX Kernel) with debug output.
                Debug level configured in Net_Debug.c configuration file.
                Use HyperTerminal to view output messages and select
                the COM# Windows has assigned to the Virtual COM port on
                the LM3S9B92 evaluation board. Set the serial connection 
                to 115200 baud, 8-bits, no parity, 1 stop bit and no flow
                control.

LM3S9B92 RTX:   The same example configured for RTX Kernel.
