Scribble Pad

The scribble pad provides a drawing area on the screen.  Touching the
screen will draw onto the drawing area using a selection of fundamental
colors (in other words, the seven colors produced by the three color
channels being either fully on or fully off).  Each time the screen is
touched to start a new drawing, the drawing area is erased and the next
color is selected.

This application supports remote software update over Ethernet using the
LM Flash Programmer application.  A firmware update is initiated using the
remote update request ``magic packet'' from LM Flash Programmer.

-------------------------------------------------------------------------------

Copyright (c) 2008-2011 Texas Instruments Incorporated.  All rights reserved.
Software License Agreement

Texas Instruments (TI) is supplying this software for use solely and
exclusively on TI's microcontroller products. The software is owned by
TI and/or its suppliers, and is protected under applicable copyright
laws. You may not combine this software with "viral" open-source
software in order to form a larger program.

THIS SOFTWARE IS PROVIDED "AS IS" AND WITH ALL FAULTS.
NO WARRANTIES, WHETHER EXPRESS, IMPLIED OR STATUTORY, INCLUDING, BUT
NOT LIMITED TO, IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
A PARTICULAR PURPOSE APPLY TO THIS SOFTWARE. TI SHALL NOT, UNDER ANY
CIRCUMSTANCES, BE LIABLE FOR SPECIAL, INCIDENTAL, OR CONSEQUENTIAL
DAMAGES, FOR ANY REASON WHATSOEVER.

This is part of revision 6852 of the RDK-IDM-SBC Firmware Package.
