/******************** (C) COPYRIGHT 2008 STMicroelectronics ********************
* File Name          : readme.txt
* Author             : MCD Application Team
* Version            : V2.0.1
* Date               : 06/13/2008
* Description        : Description of the FSMC NOR_CodeExecute Example.
********************************************************************************
* THE PRESENT FIRMWARE WHICH IS FOR GUIDANCE ONLY AIMS AT PROVIDING CUSTOMERS
* WITH CODING INFORMATION REGARDING THEIR PRODUCTS IN ORDER FOR THEM TO SAVE TIME.
* AS A RESULT, STMICROELECTRONICS SHALL NOT BE HELD LIABLE FOR ANY DIRECT,
* INDIRECT OR CONSEQUENTIAL DAMAGES WITH RESPECT TO ANY CLAIMS ARISING FROM THE
* CONTENT OF SUCH FIRMWARE AND/OR THE USE MADE BY CUSTOMERS OF THE CODING
* INFORMATION CONTAINED HEREIN IN CONNECTION WITH THEIR PRODUCTS.
*******************************************************************************/

Example description
===================
This directory contains a set of sources files that describes how to build an
application to be loaded into the NOR memory mounted on STM3210E-EVAL board then
execute it from internal Flash.


Directory contents
==================
 + \binary           Contains a set of sources files that build the application 
                     to be loaded into the NOR memory mounted on STM3210E-EVAL board.
 + stm32f10x_conf.h  Library Configuration file
 + stm32f10x_it.c    Interrupt handlers
 + stm32f10x_it.h    Header for stm32f10x_it.c
 + main.c            Main program


Hardware environment
====================
This example runs on STMicroelectronics STM3210B-EVAL and STM3210E-EVAL evaluation
boards and can be easily tailored to any other hardware.

    
How to use it
=============
In order to make the program work, you must do the following:
1. Program the NOR memory with the example provided in the \binary directory
2. Program the internal Flash with the code that will jump to the NOR memory to execute 
    the loaded example, for this you have to:
      - Create a project and setup all your toolchain's start-up files
      - Compile the directory content files and required Library files:
          + stm32f10x_lib.c
          + stm32f10x_gpio.c
          + stm32f10x_rcc.c
          + stm32f10x_nvic.c
          + stm32f10x_flash.c
      - Link all compiled files and load your image into target memory
      - Run the example


******************* (C) COPYRIGHT 2008 STMicroelectronics *****END OF FILE******
