/**
  @page TASKING_STM320518 TASKING Project Template for STM32F0xx devices
  
  @verbatim
  ******************* (C) COPYRIGHT 2012 STMicroelectronics ********************
  * @file    readme.txt
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-May-2012
  * @brief   This sub-directory contains all the user-modifiable files needed
  *          to create a new project linked with the STM32F0xx Standard Peripheral 
  *          Library and working with TASKING VX-toolset for ARM Cortex-M.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
   @endverbatim
 
 @par Directory contents

 - .cproject/.project: A pre-configured project file with the provided library
                       structure that produces an executable image with TASKING.

- TASKING                  : This folder contains
 
     - stm32f0xx.lsl       : This file is TASKING linker script that contains the 
                             STM32F0xx vector table and used to place program code (readonly) 
                             in internal FLASH and data (readwrite, Stack and Heap)in
                             internal SRAM. 
                             You can customize this file to your need.

     - cstart_thumb2.asm   : This file initializes the stack pointer and copy initialized
                             sections from ROM to RAM

@par How to use it ?

 - Open TASKING toolchain.
 - Click on File->Import, select General->'Existing Projects into Workspace' 
   and then click "Next". 
 - Browse to  TASKING workspace directory and select the project: 
   - STM320518_EVAL: to configure the project for STM32F0xx devices.
  - Rebuild all project files: Select the project in the "Project explorer" 
   window then click on Project->build project menu.
 - Run program: Select the project in the "Project explorer" window then click 
   Run->Debug (F11)

 @note The needed define symbols for this config are already declared in the
       preprocessor section: USE_STM320518_EVAL, STM32F0XX, USE_STDPERIPH_DRIVER 

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
