Graphics Library String Table Demonstration

This application provides a demonstration of the capabilities of the
Stellaris Graphics Library's string table functions.  A series of panels
show different implementations of features of the string table functions.
For each panel, the bottom provides a forward and back button
(when appropriate).

The first panel provides a large string with introductory text and basic
instructions for operation of the application.

The second panel shows the available languages and allows them to be
switched between English, German, Spanish and Italian.

The final panel provides instructions and information necessary to update
the board firmware via ethernet using the LM Flash Programmer application.
When the ``Update'' button is pressed, the application transfers control to
the boot loader to allow a new application image to be downloaded.  If using
a recent version of LMFlash, firmware download can also be initiated
automatically via a ``magic packet'' sent from LMFlash to the IDM-SBC.  When
this packet is received, the application transfers control to the boot
loader without any required user interaction.

-------------------------------------------------------------------------------

Copyright (c) 2008-2011 Texas Instruments Incorporated.  All rights reserved.
Software License Agreement

Texas Instruments (TI) is supplying this software for use solely and
exclusively on TI's microcontroller products. The software is owned by
TI and/or its suppliers, and is protected under applicable copyright
laws. You may not combine this software with "viral" open-source
software in order to form a larger program.

THIS SOFTWARE IS PROVIDED "AS IS" AND WITH ALL FAULTS.
NO WARRANTIES, WHETHER EXPRESS, IMPLIED OR STATUTORY, INCLUDING, BUT
NOT LIMITED TO, IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
A PARTICULAR PURPOSE APPLY TO THIS SOFTWARE. TI SHALL NOT, UNDER ANY
CIRCUMSTANCES, BE LIABLE FOR SPECIAL, INCIDENTAL, OR CONSEQUENTIAL
DAMAGES, FOR ANY REASON WHATSOEVER.

This is part of revision 6852 of the RDK-IDM-SBC Firmware Package.
