
     Davicom DM9000 WinCE.net Driver v3.2.7 Release Note


    The Davicom DM9000 NDIS CE miniport device driver is used to be 
the network component of the Microsoft WinCE.net enables hardware
containing Davicom's fast ethernet controller 'DM9000'.
    This file describes the procedures of the driver installation. Note that
this is not written for end-users.

CONTENTS:

    Readme.txt      -   This file
    dm9000.msi		-	The binary release file


1. Installation

	Run the dm9000.msi to install the binary release. 
	The package	contains the following files.
	
	$(_winceroot)\public\common\oak\lib\x86\debug\dm9000.def
	$(_winceroot)\public\common\oak\lib\x86\debug\dm9000.lib
	$(_winceroot)\public\common\oak\lib\x86\debug\dm9000.pdb
	$(_winceroot)\public\common\oak\lib\x86\retail\dm9000.def
	$(_winceroot)\public\common\oak\lib\x86\retail\dm9000.lib
	$(_winceroot)\public\common\oak\lib\x86\retail\dm9000.pdb
	$(_winceroot)\public\common\oak\files\dm9000\config.bi_
	$(_winceroot)\public\common\oak\files\dm9000\project.bi_
	$(_winceroot)\public\common\oak\files\dm9000\project.re_
	
2. Platform Configuration
2.1 Add 'dm9000' target to the root makefile.
	Open the file $(_winceroot)\public\common\cesysgen\makefile
	Append 'dm9000' to all 'dc21x4' rules or dependencies.
	
2.2 Modify your cesysgen.bat, to add 'dm9000' to CE_MODULES
	<e.g.>
	$(_winceroot)\public\<your project>\wince400\cepc\oak\misc\cesysgen.bat
	
	set CE_MODULES=dm9000 %CE_MODULES%
	
2.3 Modify your project.bib for module definition

	<e.g.>
	MODULES
	dm9000.dll       $(_FLATRELEASEDIR)\dm9000.dll              NK  SH

3. Driver Configuration
3.1	In the file project.reg, add the following registry values.
	<e.g.>
	
         [HKEY_LOCAL_MACHINE\Comm\DM9CE]
             "DisplayName"="DM9000 Fast Ethernet Adapter"
             "Group"="NDIS"
             "ImagePath"="dm9000.dll"

         [HKEY_LOCAL_MACHINE\Comm\DM9CE\Linkage]
             "Route"=multi_sz:"DM9CE1"

         [HKEY_LOCAL_MACHINE\Comm\DM9CE1]
             "DisplayName"="DM9000 Fast Ethernet Adapter"
             "Group"="NDIS"
             "ImagePath"="dm9000.dll"

         [HKEY_LOCAL_MACHINE\Comm\Tcpip\Linkage]
             "Bind"="dm9pci1"

         [HKEY_LOCAL_MACHINE\Comm\DM9CE1\Parms]
			 "BusNumber"=dword:0
			 "BusType"=dword:1
             "XmitBuffer"=dword:A
             "RecvBuffer"=dword:20

         [HKEY_LOCAL_MACHINE\Comm\DM9CE1\Parms\TcpIp]
             "EnableDHCP"=dword:0
             "UseZeroBroadcast"=dword:0
             "DefaultGateway"="x.x.x.x."
             "IpAddress"="x.x.x.x."
             "Subnetmask"="x.x.x.x"
             "DNS"="x.x.x.x"
             "WINS"="x.x.x.x"

3.2 TCP/IP configurations

3.2.1 EnableDHCP
	Set 1 for DHCP enable, 0 for disable.
	
3.2.2 UseZeroBroadcast
	Set 1 for use zero broadcast, 0 for not.
	
3.2.3 DefaultGateway
	Specify your gateway address in x.x.x.x format.
	
3.2.4 IpAddress
	Specify your IP address in x.x.x.x format.
	
3.2.5 Subnetmask
	Specify your subnet mask in x.x.x.x format.
	
3.2.6 DNS
	Specify your domain name server's address in x.x.x.x format.
	
3.2.7 WINS
	Specify your WINS server's address in x.x.x.x format.
	

------------------------------------------------------------------------------
All trademarks or brand names mentioned are trademarks and registered trademarks
of their respective companies.
